# `socket` --- 底层网络接口

源代码: Lib/socket.py

这个模块提供了访问 BSD 套接字 的接口。在所有现代 Unix 系统、Windows、macOS 和其他一些平台上可用。

注解

一些行为可能因平台不同而异，因为调用的是操作系统的套接字API。

这个Python接口是用Python的面向对象风格对Unix系统调用和套接字库接口的直译：函数 `socket()` 返回一个 套接字对象 ，其方法是对各种套接字系统调用的实现。形参类型一般与C接口相比更高级：例如在Python文件 `read()` 和 `write()` 操作中，接收操作的缓冲区分配是自动的，发送操作的缓冲区长度是隐式的。

参见

模块 `socketserver`

  用于简化网络服务端编写的类。

模块 `ssl`

  套接字对象的TLS/SSL封装。

## 套接字协议族

根据系统以及构建选项，此模块提供了各种套接字协议簇。

特定的套接字对象需要的地址格式将根据此套接字对象被创建时指定的地址族被自动选择。套接字地址表示如下：

- 一个绑定在文件系统节点上的 `AF_UNIX` 套接字的地址表示为一个字符串，使用文件系统字符编码和 `'surrogateescape'` 错误回调方法（see PEP 383）。一个地址在 Linux 的抽象命名空间被返回为带有初始的 null 字节的 字节类对象 ；注意在这个命名空间种的套接字可能与普通文件系统套接字通信，所以打算运行在 Linux 上的程序可能需要解决两种地址类型。当传递为参数时，一个字符串或字节类对象可以用于任一类型的地址。

  > 在 3.3 版更改: 之前，`AF_UNIX` 套接字路径被假设使用 UTF-8 编码。

  > 在 3.5 版更改: 现在支持可写的 字节类对象。

- 一对 `(host, port)` 被用于 `AF_INET` 地址族，host 是一个表示为互联网域名表示法之内的主机名或者一个 IPv4 地址的字符串，例如 `'daring.cwi.nl'` 或 `'100.50.200.5'`，port 是一个整数。

  - 对于 IPv4 地址，有两种可接受的特殊形式被用来代替一个主机地址： `''` 代表 `INADDR_ANY`，用来绑定到所有接口；字符串 `'<broadcast>'` 代表 `INADDR_BROADCAST`。此行为不兼容 IPv6，因此，如果你的 Python 程序打算支持 IPv6，则可能需要避开这些。

- For `AF_INET6` address family, a four-tuple `(host, port, flowinfo, scope_id)` is used, where flowinfo and scope_id represent the `sin6_flowinfo` and `sin6_scope_id` members in `struct sockaddr_in6` in C. For `socket` module methods, flowinfo and scope_id can be omitted just for backward compatibility. Note, however, omission of scope_id can cause problems in manipulating scoped IPv6 addresses.

  在 3.7 版更改: For multicast addresses (with scope_id meaningful) address may not contain `%scope_id` (or `zone id`) part. This information is superfluous and may be safely omitted (recommended).

- `AF_NETLINK` 套接字由一对 `(pid, groups)` 表示。

- 指定 `AF_TIPC` 地址族可以使用仅 Linux 支持的 TIPC 协议。TIPC 是一种开放的、非基于 IP 的网络协议，旨在用于集群计算环境。其地址用元组表示，其中的字段取决于地址类型。一般元组形式为 `(addr_type, v1, v2, v3 [, scope])`，其中：

  - addr_type 取 `TIPC_ADDR_NAMESEQ`、`TIPC_ADDR_NAME` 或 `TIPC_ADDR_ID` 中的一个。

  - scope 取 `TIPC_ZONE_SCOPE`、`TIPC_CLUSTER_SCOPE` 和 `TIPC_NODE_SCOPE` 中的一个。

  - 如果 addr_type 为 `TIPC_ADDR_NAME`，那么 v1 是服务器类型，v2 是端口标识符，v3 应为 0。

    如果 addr_type 为 `TIPC_ADDR_NAMESEQ`，那么 v1 是服务器类型，v2 是端口号下限，而 v3 是端口号上限。

    如果 addr_type 为 `TIPC_ADDR_ID`，那么 v1 是节点 (node)，v2 是 ref，v3 应为 0。

- `AF_CAN` 地址族使用元组 `(interface, )`，其中 interface 是表示网络接口名称的字符串，如 `'can0'`。网络接口名 `''` 可以用于接收本族所有网络接口的数据包。

  - `CAN_ISOTP` 协议接受一个元组 `(interface, rx_addr, tx_addr)`，其中两个额外参数都是无符号长整数，都表示 CAN 标识符（标准或扩展标识符）。

- `PF_SYSTEM` 协议簇的 `SYSPROTO_CONTROL` 协议接受一个字符串或元组 `(id, unit)`。其中字符串是内核控件的名称，该控件使用动态分配的 ID。而如果 ID 和内核控件的单元 (unit) 编号都已知，或使用了已注册的 ID，可以采用元组。

  3.3 新版功能.

- `AF_BLUETOOTH` supports the following protocols and address formats:

  - `BTPROTO_L2CAP` accepts `(bdaddr, psm)` where `bdaddr` is the Bluetooth address as a string and `psm` is an integer.

  - `BTPROTO_RFCOMM` accepts `(bdaddr, channel)` where `bdaddr` is the Bluetooth address as a string and `channel` is an integer.

  - `BTPROTO_HCI` accepts `(device_id,)` where `device_id` is either an integer or a string with the Bluetooth address of the interface. (This depends on your OS; NetBSD and DragonFlyBSD expect a Bluetooth address while everything else expects an integer.)

    在 3.2 版更改: NetBSD and DragonFlyBSD support added.

  - `BTPROTO_SCO` accepts `bdaddr` where `bdaddr` is a `bytes` object containing the Bluetooth address in a string format. (ex. `b'12:23:34:45:56:67'`) This protocol is not supported under FreeBSD.

- `AF_ALG` is a Linux-only socket based interface to Kernel cryptography. An algorithm socket is configured with a tuple of two to four elements `(type, name [, feat [, mask]])`, where:

  - type is the algorithm type as string, e.g. `aead`, `hash`, `skcipher` or `rng`.

  - name is the algorithm name and operation mode as string, e.g. `sha256`, `hmac(sha256)`, `cbc(aes)` or `drbg_nopr_ctr_aes256`.

  - feat and mask are unsigned 32bit integers.

  Availability: Linux 2.6.38, some algorithm types require more recent Kernels.

  3.6 新版功能.

- `AF_VSOCK` allows communication between virtual machines and their hosts. The sockets are represented as a `(CID, port)` tuple where the context ID or CID and port are integers.

  Availability: Linux >= 4.8 QEMU >= 2.8 ESX >= 4.0 ESX Workstation >= 6.5.

  3.7 新版功能.

- `AF_PACKET` is a low-level interface directly to network devices. The packets are represented by the tuple `(ifname, proto[, pkttype[, hatype[, addr]]])` where:

  - ifname - String specifying the device name.

  - proto - An in network-byte-order integer specifying the Ethernet protocol number.

  - pkttype - Optional integer specifying the packet type:

    - `PACKET_HOST` (the default) - Packet addressed to the local host.

    - `PACKET_BROADCAST` - Physical-layer broadcast packet.

    - `PACKET_MULTIHOST` - Packet sent to a physical-layer multicast address.

    - `PACKET_OTHERHOST` - Packet to some other host that has been caught by a device driver in promiscuous mode.

    - `PACKET_OUTGOING` - Packet originating from the local host that is looped back to a packet socket.

  - hatype - Optional integer specifying the ARP hardware address type.

  - addr - Optional bytes-like object specifying the hardware physical address, whose interpretation depends on the device.

- `AF_QIPCRTR` is a Linux-only socket based interface for communicating with services running on co-processors in Qualcomm platforms. The address family is represented as a `(node, port)` tuple where the node and port are non-negative integers.

  3.8 新版功能.

- `IPPROTO_UDPLITE` is a variant of UDP which allows you to specify what portion of a packet is covered with the checksum. It adds two socket options that you can change. `self.setsockopt(IPPROTO_UDPLITE, UDPLITE_SEND_CSCOV, length)` will change what portion of outgoing packets are covered by the checksum and `self.setsockopt(IPPROTO_UDPLITE, UDPLITE_RECV_CSCOV, length)` will filter out packets which cover too little of their data. In both cases `length` should be in `range(8, 2**16, 8)`.

  Such a socket should be constructed with `socket(AF_INET, SOCK_DGRAM, IPPROTO_UDPLITE)` for IPv4 or `socket(AF_INET6, SOCK_DGRAM, IPPROTO_UDPLITE)` for IPv6.

  Availability: Linux >= 2.6.20, FreeBSD >= 10.1-RELEASE

  3.9 新版功能.

如果你在 IPv4/v6 套接字地址的 host 部分中使用了一个主机名，此程序可能会表现不确定行为，因为 Python 使用 DNS 解析返回的第一个地址。套接字地址在实际的 IPv4/v6 中以不同方式解析，根据 DNS 解析和/或 host 配置。为了确定行为，在 host 部分中使用数字的地址。

所有的错误都抛出异常。对于无效的参数类型和内存溢出异常情况可能抛出普通异常；从 Python 3.3 开始，与套接字或地址语义有关的错误抛出 `OSError` 或它的子类之一（常用 `socket.error`）。

可以用 `setblocking()` 设置非阻塞模式。一个基于超时的 generalization 通过 `settimeout()` 支持。

## 模块内容

`socket` 模块导出以下元素。

### 异常

exception `socket.``error`

  一个被弃用的 `OSError` 的别名。

  在 3.3 版更改: 根据 PEP 3151，这个类是 `OSError` 的别名。

exception `socket.``herror`

  A subclass of `OSError`, this exception is raised for address-related errors, i.e. for functions that use h_errno in the POSIX C API, including `gethostbyname_ex()` and `gethostbyaddr()`. The accompanying value is a pair `(h_errno, string)` representing an error returned by a library call. h_errno is a numeric value, while string represents the description of h_errno, as returned by the `hstrerror()` C function.

  在 3.3 版更改: This class was made a subclass of `OSError`.

exception `socket.``gaierror`

  A subclass of `OSError`, this exception is raised for address-related errors by `getaddrinfo()` and `getnameinfo()`. The accompanying value is a pair `(error, string)` representing an error returned by a library call. string represents the description of error, as returned by the `gai_strerror()` C function. The numeric error value will match one of the `EAI_*` constants defined in this module.

  在 3.3 版更改: This class was made a subclass of `OSError`.

exception `socket.``timeout`

  A subclass of `OSError`, this exception is raised when a timeout occurs on a socket which has had timeouts enabled via a prior call to `settimeout()` (or implicitly through `setdefaulttimeout()`). The accompanying value is a string whose value is currently always "timed out".

  在 3.3 版更改: This class was made a subclass of `OSError`.

### 常数

> The AF_* and SOCK_* constants are now `AddressFamily` and `SocketKind` `IntEnum` collections.

> 3.4 新版功能.

`socket.``AF_UNIX`
`socket.``AF_INET`
`socket.``AF_INET6`

  These constants represent the address (and protocol) families, used for the first argument to `socket()`. If the `AF_UNIX` constant is not defined then this protocol is unsupported. More constants may be available depending on the system.

`socket.``SOCK_STREAM`
`socket.``SOCK_DGRAM`
`socket.``SOCK_RAW`
`socket.``SOCK_RDM`
`socket.``SOCK_SEQPACKET`

  These constants represent the socket types, used for the second argument to `socket()`. More constants may be available depending on the system. (Only `SOCK_STREAM` and `SOCK_DGRAM` appear to be generally useful.)

`socket.``SOCK_CLOEXEC`
`socket.``SOCK_NONBLOCK`

  These two constants, if defined, can be combined with the socket types and allow you to set some flags atomically (thus avoiding possible race conditions and the need for separate calls).

  参见

  Secure File Descriptor Handling for a more thorough explanation.

  Availability: Linux >= 2.6.27.

  3.2 新版功能.

`SO_*`
`socket.``SOMAXCONN`
`MSG_*`
`SOL_*`
`SCM_*`
`IPPROTO_*`
`IPPORT_*`
`INADDR_*`
`IP_*`
`IPV6_*`
`EAI_*`
`AI_*`
`NI_*`
`TCP_*`

  Many constants of these forms, documented in the Unix documentation on sockets and/or the IP protocol, are also defined in the socket module. They are generally used in arguments to the `setsockopt()` and `getsockopt()` methods of socket objects. In most cases, only those symbols that are defined in the Unix header files are defined; for a few symbols, default values are provided.

  在 3.6 版更改: `SO_DOMAIN`, `SO_PROTOCOL`, `SO_PEERSEC`, `SO_PASSSEC`, `TCP_USER_TIMEOUT`, `TCP_CONGESTION` were added.

  在 3.6.5 版更改: On Windows, `TCP_FASTOPEN`, `TCP_KEEPCNT` appear if run-time Windows supports.

  在 3.7 版更改: `TCP_NOTSENT_LOWAT` was added.

  On Windows, `TCP_KEEPIDLE`, `TCP_KEEPINTVL` appear if run-time Windows supports.

`socket.``AF_CAN`
`socket.``PF_CAN`
`SOL_CAN_*`
`CAN_*`

  Many constants of these forms, documented in the Linux documentation, are also defined in the socket module.

  Availability: Linux >= 2.6.25.

  3.3 新版功能.

`socket.``CAN_BCM`
`CAN_BCM_*`

  CAN_BCM, in the CAN protocol family, is the broadcast manager (BCM) protocol. Broadcast manager constants, documented in the Linux documentation, are also defined in the socket module.

  Availability: Linux >= 2.6.25.

  注解

  The `CAN_BCM_CAN_FD_FRAME` flag is only available on Linux >= 4.8.

  3.4 新版功能.

`socket.``CAN_RAW_FD_FRAMES`

  Enables CAN FD support in a CAN_RAW socket. This is disabled by default. This allows your application to send both CAN and CAN FD frames; however, you must accept both CAN and CAN FD frames when reading from the socket.

  This constant is documented in the Linux documentation.

  Availability: Linux >= 3.6.

  3.5 新版功能.

`socket.``CAN_RAW_JOIN_FILTERS`

  Joins the applied CAN filters such that only CAN frames that match all given CAN filters are passed to user space.

  This constant is documented in the Linux documentation.

  Availability: Linux >= 4.1.

  3.9 新版功能.

`socket.``CAN_ISOTP`

  CAN_ISOTP, in the CAN protocol family, is the ISO-TP (ISO 15765-2) protocol. ISO-TP constants, documented in the Linux documentation.

  Availability: Linux >= 2.6.25.

  3.7 新版功能.

`socket.``AF_PACKET`
`socket.``PF_PACKET`
`PACKET_*`

  Many constants of these forms, documented in the Linux documentation, are also defined in the socket module.

  Availability: Linux >= 2.2.

`socket.``AF_RDS`
`socket.``PF_RDS`
`socket.``SOL_RDS`
`RDS_*`

  Many constants of these forms, documented in the Linux documentation, are also defined in the socket module.

  Availability: Linux >= 2.6.30.

  3.3 新版功能.

`socket.``SIO_RCVALL`
`socket.``SIO_KEEPALIVE_VALS`
`socket.``SIO_LOOPBACK_FAST_PATH`
`RCVALL_*`

  Constants for Windows' WSAIoctl(). The constants are used as arguments to the `ioctl()` method of socket objects.

  在 3.6 版更改: `SIO_LOOPBACK_FAST_PATH` was added.

`TIPC_*`

  TIPC related constants, matching the ones exported by the C socket API. See the TIPC documentation for more information.

`socket.``AF_ALG`
`socket.``SOL_ALG`
`ALG_*`

  Constants for Linux Kernel cryptography.

  Availability: Linux >= 2.6.38.

  3.6 新版功能.

`socket.``AF_VSOCK`
`socket.``IOCTL_VM_SOCKETS_GET_LOCAL_CID`
`VMADDR*`
`SO_VM*`

  Constants for Linux host/guest communication.

  Availability: Linux >= 4.8.

  3.7 新版功能.

`socket.``AF_LINK`

  Availability: BSD, OSX.

  3.4 新版功能.

`socket.``has_ipv6`

  This constant contains a boolean value which indicates if IPv6 is supported on this platform.

`socket.``BDADDR_ANY`
`socket.``BDADDR_LOCAL`

  These are string constants containing Bluetooth addresses with special meanings. For example, `BDADDR_ANY` can be used to indicate any address when specifying the binding socket with `BTPROTO_RFCOMM`.

`socket.``HCI_FILTER`
`socket.``HCI_TIME_STAMP`
`socket.``HCI_DATA_DIR`

  For use with `BTPROTO_HCI`. `HCI_FILTER` is not available for NetBSD or DragonFlyBSD. `HCI_TIME_STAMP` and `HCI_DATA_DIR` are not available for FreeBSD, NetBSD, or DragonFlyBSD.

`socket.``AF_QIPCRTR`

  Constant for Qualcomm's IPC router protocol, used to communicate with service providing remote processors.

  Availability: Linux >= 4.7.

### 函数

#### Creating sockets

The following functions all create socket objects.

`socket.``socket`(family=AF_INET, type=SOCK_STREAM, proto=0, fileno=None)

  Create a new socket using the given address family, socket type and protocol number. The address family should be `AF_INET` (the default), `AF_INET6`, `AF_UNIX`, `AF_CAN`, `AF_PACKET`, or `AF_RDS`. The socket type should be `SOCK_STREAM` (the default), `SOCK_DGRAM`, `SOCK_RAW` or perhaps one of the other `SOCK_` constants. The protocol number is usually zero and may be omitted or in the case where the address family is `AF_CAN` the protocol should be one of `CAN_RAW`, `CAN_BCM` or `CAN_ISOTP`.

  If fileno is specified, the values for family, type, and proto are auto-detected from the specified file descriptor. Auto-detection can be overruled by calling the function with explicit family, type, or proto arguments. This only affects how Python represents e.g. the return value of `socket.getpeername()` but not the actual OS resource. Unlike `socket.fromfd()`, fileno will return the same socket and not a duplicate. This may help close a detached socket using `socket.close()`.

  The newly created socket is non-inheritable.

  Raises an auditing event `socket.__new__` with arguments `self`, `family`, `type`, `protocol`.

  在 3.3 版更改: The AF_CAN family was added. The AF_RDS family was added.

  在 3.4 版更改: The CAN_BCM protocol was added.

  在 3.4 版更改: The returned socket is now non-inheritable.

  在 3.7 版更改: The CAN_ISOTP protocol was added.

  在 3.7 版更改: When `SOCK_NONBLOCK` or `SOCK_CLOEXEC` bit flags are applied to type they are cleared, and `socket.type` will not reflect them. They are still passed to the underlying system socket() call. Therefore,

      sock = socket.socket(
          socket.AF_INET,
          socket.SOCK_STREAM | socket.SOCK_NONBLOCK)

  will still create a non-blocking socket on OSes that support `SOCK_NONBLOCK`, but `sock.type` will be set to `socket.SOCK_STREAM`.

`socket.``socketpair`([family[, type[, proto]]])

  Build a pair of connected socket objects using the given address family, socket type, and protocol number. Address family, socket type, and protocol number are as for the `socket()` function above. The default family is `AF_UNIX` if defined on the platform; otherwise, the default is `AF_INET`.

  The newly created sockets are non-inheritable.

  在 3.2 版更改: The returned socket objects now support the whole socket API, rather than a subset.

  在 3.4 版更改: The returned sockets are now non-inheritable.

  在 3.5 版更改: Windows support added.

`socket.``create_connection`(address[, timeout[, source_address]])

  Connect to a TCP service listening on the Internet address (a 2-tuple `(host, port)`), and return the socket object. This is a higher-level function than `socket.connect()`: if host is a non-numeric hostname, it will try to resolve it for both `AF_INET` and `AF_INET6`, and then try to connect to all possible addresses in turn until a connection succeeds. This makes it easy to write clients that are compatible to both IPv4 and IPv6.

  Passing the optional timeout parameter will set the timeout on the socket instance before attempting to connect. If no timeout is supplied, the global default timeout setting returned by `getdefaulttimeout()` is used.

  If supplied, source_address must be a 2-tuple `(host, port)` for the socket to bind to as its source address before connecting. If host or port are '' or 0 respectively the OS default behavior will be used.

  在 3.2 版更改: 添加了 source_address。

`socket.``create_server`(address, *, family=AF_INET, backlog=None, reuse_port=False, dualstack_ipv6=False)

  Convenience function which creates a TCP socket bound to address (a 2-tuple `(host, port)`) and return the socket object.

  family should be either `AF_INET` or `AF_INET6`. backlog is the queue size passed to `socket.listen()`; when `0` a default reasonable value is chosen. reuse_port dictates whether to set the `SO_REUSEPORT` socket option.

  If dualstack_ipv6 is true and the platform supports it the socket will be able to accept both IPv4 and IPv6 connections, else it will raise `ValueError`. Most POSIX platforms and Windows are supposed to support this functionality. When this functionality is enabled the address returned by `socket.getpeername()` when an IPv4 connection occurs will be an IPv6 address represented as an IPv4-mapped IPv6 address. If dualstack_ipv6 is false it will explicitly disable this functionality on platforms that enable it by default (e.g. Linux). This parameter can be used in conjunction with `has_dualstack_ipv6()`:

      import socket

      addr = ("", 8080)  # all interfaces, port 8080
      if socket.has_dualstack_ipv6():
          s = socket.create_server(addr, family=socket.AF_INET6, dualstack_ipv6=True)
      else:
          s = socket.create_server(addr)

  注解

  On POSIX platforms the `SO_REUSEADDR` socket option is set in order to immediately reuse previous sockets which were bound on the same address and remained in TIME_WAIT state.

  3.8 新版功能.

`socket.``has_dualstack_ipv6`()

  Return `True` if the platform supports creating a TCP socket which can handle both IPv4 and IPv6 connections.

  3.8 新版功能.

`socket.``fromfd`(fd, family, type, proto=0)

  Duplicate the file descriptor fd (an integer as returned by a file object's `fileno()` method) and build a socket object from the result. Address family, socket type and protocol number are as for the `socket()` function above. The file descriptor should refer to a socket, but this is not checked --- subsequent operations on the object may fail if the file descriptor is invalid. This function is rarely needed, but can be used to get or set socket options on a socket passed to a program as standard input or output (such as a server started by the Unix inet daemon). The socket is assumed to be in blocking mode.

  The newly created socket is non-inheritable.

  在 3.4 版更改: The returned socket is now non-inheritable.

`socket.``fromshare`(data)

  Instantiate a socket from data obtained from the `socket.share()` method. The socket is assumed to be in blocking mode.

  可用性: Windows。

  3.3 新版功能.

`socket.``SocketType`

  This is a Python type object that represents the socket object type. It is the same as `type(socket(...))`.

#### 其他功能

The `socket` module also offers various network-related services:

`socket.``close`(fd)

  Close a socket file descriptor. This is like `os.close()`, but for sockets. On some platforms (most noticeable Windows) `os.close()` does not work for socket file descriptors.

  3.7 新版功能.

`socket.``getaddrinfo`(host, port, family=0, type=0, proto=0, flags=0)

  Translate the host/port argument into a sequence of 5-tuples that contain all the necessary arguments for creating a socket connected to that service. host is a domain name, a string representation of an IPv4/v6 address or `None`. port is a string service name such as `'http'`, a numeric port number or `None`. By passing `None` as the value of host and port, you can pass `NULL` to the underlying C API.

  The family, type and proto arguments can be optionally specified in order to narrow the list of addresses returned. Passing zero as a value for each of these arguments selects the full range of results. The flags argument can be one or several of the `AI_*` constants, and will influence how results are computed and returned. For example, `AI_NUMERICHOST` will disable domain name resolution and will raise an error if host is a domain name.

  The function returns a list of 5-tuples with the following structure:

  `(family, type, proto, canonname, sockaddr)`

  In these tuples, family, type, proto are all integers and are meant to be passed to the `socket()` function. canonname will be a string representing the canonical name of the host if `AI_CANONNAME` is part of the flags argument; else canonname will be empty. sockaddr is a tuple describing a socket address, whose format depends on the returned family (a `(address, port)` 2-tuple for `AF_INET`, a `(address, port, flowinfo, scope_id)` 4-tuple for `AF_INET6`), and is meant to be passed to the `socket.connect()` method.

  Raises an auditing event `socket.getaddrinfo` with arguments `host`, `port`, `family`, `type`, `protocol`.

  The following example fetches address information for a hypothetical TCP connection to `example.org` on port 80 (results may differ on your system if IPv6 isn't enabled):

      >>> socket.getaddrinfo("example.org", 80, proto=socket.IPPROTO_TCP)
      [(<AddressFamily.AF_INET6: 10>, <SocketType.SOCK_STREAM: 1>,
       6, '', ('2606:2800:220:1:248:1893:25c8:1946', 80, 0, 0)),
       (<AddressFamily.AF_INET: 2>, <SocketType.SOCK_STREAM: 1>,
       6, '', ('93.184.216.34', 80))]

  在 3.2 版更改: parameters can now be passed using keyword arguments.

  在 3.7 版更改: for IPv6 multicast addresses, string representing an address will not contain `%scope_id` part.

`socket.``getfqdn`([name])

  Return a fully qualified domain name for name. If name is omitted or empty, it is interpreted as the local host. To find the fully qualified name, the hostname returned by `gethostbyaddr()` is checked, followed by aliases for the host, if available. The first name which includes a period is selected. In case no fully qualified domain name is available, the hostname as returned by `gethostname()` is returned.

`socket.``gethostbyname`(hostname)

  Translate a host name to IPv4 address format. The IPv4 address is returned as a string, such as `'100.50.200.5'`. If the host name is an IPv4 address itself it is returned unchanged. See `gethostbyname_ex()` for a more complete interface. `gethostbyname()` does not support IPv6 name resolution, and `getaddrinfo()` should be used instead for IPv4/v6 dual stack support.

  Raises an auditing event `socket.gethostbyname` with argument `hostname`.

`socket.``gethostbyname_ex`(hostname)

  Translate a host name to IPv4 address format, extended interface. Return a triple `(hostname, aliaslist, ipaddrlist)` where hostname is the primary host name responding to the given ip_address, aliaslist is a (possibly empty) list of alternative host names for the same address, and ipaddrlist is a list of IPv4 addresses for the same interface on the same host (often but not always a single address). `gethostbyname_ex()` does not support IPv6 name resolution, and `getaddrinfo()` should be used instead for IPv4/v6 dual stack support.

  Raises an auditing event `socket.gethostbyname` with argument `hostname`.

`socket.``gethostname`()

  Return a string containing the hostname of the machine where the Python interpreter is currently executing.

  Raises an auditing event `socket.gethostname` with no arguments.

  Note: `gethostname()` doesn't always return the fully qualified domain name; use `getfqdn()` for that.

`socket.``gethostbyaddr`(ip_address)

  Return a triple `(hostname, aliaslist, ipaddrlist)` where hostname is the primary host name responding to the given ip_address, aliaslist is a (possibly empty) list of alternative host names for the same address, and ipaddrlist is a list of IPv4/v6 addresses for the same interface on the same host (most likely containing only a single address). To find the fully qualified domain name, use the function `getfqdn()`. `gethostbyaddr()` supports both IPv4 and IPv6.

  Raises an auditing event `socket.gethostbyaddr` with argument `ip_address`.

`socket.``getnameinfo`(sockaddr, flags)

  Translate a socket address sockaddr into a 2-tuple `(host, port)`. Depending on the settings of flags, the result can contain a fully-qualified domain name or numeric address representation in host. Similarly, port can contain a string port name or a numeric port number.

  For IPv6 addresses, `%scope_id` is appended to the host part if sockaddr contains meaningful scope_id. Usually this happens for multicast addresses.

  For more information about flags you can consult getnameinfo(3).

  Raises an auditing event `socket.getnameinfo` with argument `sockaddr`.

`socket.``getprotobyname`(protocolname)

  Translate an Internet protocol name (for example, `'icmp'`) to a constant suitable for passing as the (optional) third argument to the `socket()` function. This is usually only needed for sockets opened in "raw" mode (`SOCK_RAW`); for the normal socket modes, the correct protocol is chosen automatically if the protocol is omitted or zero.

`socket.``getservbyname`(servicename[, protocolname])

  Translate an Internet service name and protocol name to a port number for that service. The optional protocol name, if given, should be `'tcp'` or `'udp'`, otherwise any protocol will match.

  Raises an auditing event `socket.getservbyname` with arguments `servicename`, `protocolname`.

`socket.``getservbyport`(port[, protocolname])

  Translate an Internet port number and protocol name to a service name for that service. The optional protocol name, if given, should be `'tcp'` or `'udp'`, otherwise any protocol will match.

  Raises an auditing event `socket.getservbyport` with arguments `port`, `protocolname`.

`socket.``ntohl`(x)

  Convert 32-bit positive integers from network to host byte order. On machines where the host byte order is the same as network byte order, this is a no-op; otherwise, it performs a 4-byte swap operation.

`socket.``ntohs`(x)

  Convert 16-bit positive integers from network to host byte order. On machines where the host byte order is the same as network byte order, this is a no-op; otherwise, it performs a 2-byte swap operation.

  3.7 版后已移除: In case x does not fit in 16-bit unsigned integer, but does fit in a positive C int, it is silently truncated to 16-bit unsigned integer. This silent truncation feature is deprecated, and will raise an exception in future versions of Python.

`socket.``htonl`(x)

  Convert 32-bit positive integers from host to network byte order. On machines where the host byte order is the same as network byte order, this is a no-op; otherwise, it performs a 4-byte swap operation.

`socket.``htons`(x)

  Convert 16-bit positive integers from host to network byte order. On machines where the host byte order is the same as network byte order, this is a no-op; otherwise, it performs a 2-byte swap operation.

  3.7 版后已移除: In case x does not fit in 16-bit unsigned integer, but does fit in a positive C int, it is silently truncated to 16-bit unsigned integer. This silent truncation feature is deprecated, and will raise an exception in future versions of Python.

`socket.``inet_aton`(ip_string)

  Convert an IPv4 address from dotted-quad string format (for example, '123.45.67.89') to 32-bit packed binary format, as a bytes object four characters in length. This is useful when conversing with a program that uses the standard C library and needs objects of type `struct in_addr`, which is the C type for the 32-bit packed binary this function returns.

  `inet_aton()` also accepts strings with less than three dots; see the Unix manual page inet(3) for details.

  If the IPv4 address string passed to this function is invalid, `OSError` will be raised. Note that exactly what is valid depends on the underlying C implementation of `inet_aton()`.

  `inet_aton()` does not support IPv6, and `inet_pton()` should be used instead for IPv4/v6 dual stack support.

`socket.``inet_ntoa`(packed_ip)

  Convert a 32-bit packed IPv4 address (a bytes-like object four bytes in length) to its standard dotted-quad string representation (for example, '123.45.67.89'). This is useful when conversing with a program that uses the standard C library and needs objects of type `struct in_addr`, which is the C type for the 32-bit packed binary data this function takes as an argument.

  If the byte sequence passed to this function is not exactly 4 bytes in length, `OSError` will be raised. `inet_ntoa()` does not support IPv6, and `inet_ntop()` should be used instead for IPv4/v6 dual stack support.

  在 3.5 版更改: 现在支持可写的 字节类对象。

`socket.``inet_pton`(address_family, ip_string)

  Convert an IP address from its family-specific string format to a packed, binary format. `inet_pton()` is useful when a library or network protocol calls for an object of type `struct in_addr` (similar to `inet_aton()`) or `struct in6_addr`.

  Supported values for address_family are currently `AF_INET` and `AF_INET6`. If the IP address string ip_string is invalid, `OSError` will be raised. Note that exactly what is valid depends on both the value of address_family and the underlying implementation of `inet_pton()`.

  Availability: Unix (maybe not all platforms), Windows.

  在 3.4 版更改: Windows support added

`socket.``inet_ntop`(address_family, packed_ip)

  Convert a packed IP address (a bytes-like object of some number of bytes) to its standard, family-specific string representation (for example, `'7.10.0.5'` or `'5aef:2b::8'`). `inet_ntop()` is useful when a library or network protocol returns an object of type `struct in_addr` (similar to `inet_ntoa()`) or `struct in6_addr`.

  Supported values for address_family are currently `AF_INET` and `AF_INET6`. If the bytes object packed_ip is not the correct length for the specified address family, `ValueError` will be raised. `OSError` is raised for errors from the call to `inet_ntop()`.

  Availability: Unix (maybe not all platforms), Windows.

  在 3.4 版更改: Windows support added

  在 3.5 版更改: 现在支持可写的 字节类对象。

`socket.``CMSG_LEN`(length)

  Return the total length, without trailing padding, of an ancillary data item with associated data of the given length. This value can often be used as the buffer size for `recvmsg()` to receive a single item of ancillary data, but RFC 3542 requires portable applications to use `CMSG_SPACE()` and thus include space for padding, even when the item will be the last in the buffer. Raises `OverflowError` if length is outside the permissible range of values.

  Availability: most Unix platforms, possibly others.

  3.3 新版功能.

`socket.``CMSG_SPACE`(length)

  Return the buffer size needed for `recvmsg()` to receive an ancillary data item with associated data of the given length, along with any trailing padding. The buffer space needed to receive multiple items is the sum of the `CMSG_SPACE()` values for their associated data lengths. Raises `OverflowError` if length is outside the permissible range of values.

  Note that some systems might support ancillary data without providing this function. Also note that setting the buffer size using the results of this function may not precisely limit the amount of ancillary data that can be received, since additional data may be able to fit into the padding area.

  Availability: most Unix platforms, possibly others.

  3.3 新版功能.

`socket.``getdefaulttimeout`()

  Return the default timeout in seconds (float) for new socket objects. A value of `None` indicates that new socket objects have no timeout. When the socket module is first imported, the default is `None`.

`socket.``setdefaulttimeout`(timeout)

  Set the default timeout in seconds (float) for new socket objects. When the socket module is first imported, the default is `None`. See `settimeout()` for possible values and their respective meanings.

`socket.``sethostname`(name)

  Set the machine's hostname to name. This will raise an `OSError` if you don't have enough rights.

  Raises an auditing event `socket.sethostname` with argument `name`.

  Availability: Unix.

  3.3 新版功能.

`socket.``if_nameindex`()

  Return a list of network interface information (index int, name string) tuples. `OSError` if the system call fails.

  可用性: Unix, Windows。

  3.3 新版功能.

  在 3.8 版更改: Windows support was added.

`socket.``if_nametoindex`(if_name)

  Return a network interface index number corresponding to an interface name. `OSError` if no interface with the given name exists.

  可用性: Unix, Windows。

  3.3 新版功能.

  在 3.8 版更改: Windows support was added.

`socket.``if_indextoname`(if_index)

  Return a network interface name corresponding to an interface index number. `OSError` if no interface with the given index exists.

  可用性: Unix, Windows。

  3.3 新版功能.

  在 3.8 版更改: Windows support was added.

## Socket Objects

Socket objects have the following methods. Except for `makefile()`, these correspond to Unix system calls applicable to sockets.

在 3.2 版更改: Support for the context manager protocol was added. Exiting the context manager is equivalent to calling `close()`.

`socket.``accept`()

  Accept a connection. The socket must be bound to an address and listening for connections. The return value is a pair `(conn, address)` where conn is a new socket object usable to send and receive data on the connection, and address is the address bound to the socket on the other end of the connection.

  The newly created socket is non-inheritable.

  在 3.4 版更改: The socket is now non-inheritable.

  在 3.5 版更改: If the system call is interrupted and the signal handler does not raise an exception, the method now retries the system call instead of raising an `InterruptedError` exception (see PEP 475 for the rationale).

`socket.``bind`(address)

  Bind the socket to address. The socket must not already be bound. (The format of address depends on the address family --- see above.)

  Raises an auditing event `socket.bind` with arguments `self`, `address`.

`socket.``close`()

  Mark the socket closed. The underlying system resource (e.g. a file descriptor) is also closed when all file objects from `makefile()` are closed. Once that happens, all future operations on the socket object will fail. The remote end will receive no more data (after queued data is flushed).

  Sockets are automatically closed when they are garbage-collected, but it is recommended to `close()` them explicitly, or to use a `with` statement around them.

  在 3.6 版更改: `OSError` is now raised if an error occurs when the underlying `close()` call is made.

  注解

  `close()` releases the resource associated with a connection but does not necessarily close the connection immediately. If you want to close the connection in a timely fashion, call `shutdown()` before `close()`.

`socket.``connect`(address)

  Connect to a remote socket at address. (The format of address depends on the address family --- see above.)

  If the connection is interrupted by a signal, the method waits until the connection completes, or raise a `socket.timeout` on timeout, if the signal handler doesn't raise an exception and the socket is blocking or has a timeout. For non-blocking sockets, the method raises an `InterruptedError` exception if the connection is interrupted by a signal (or the exception raised by the signal handler).

  Raises an auditing event `socket.connect` with arguments `self`, `address`.

  在 3.5 版更改: The method now waits until the connection completes instead of raising an `InterruptedError` exception if the connection is interrupted by a signal, the signal handler doesn't raise an exception and the socket is blocking or has a timeout (see the PEP 475 for the rationale).

`socket.``connect_ex`(address)

  Like `connect(address)`, but return an error indicator instead of raising an exception for errors returned by the C-level `connect()` call (other problems, such as "host not found," can still raise exceptions). The error indicator is `0` if the operation succeeded, otherwise the value of the `errno` variable. This is useful to support, for example, asynchronous connects.

  Raises an auditing event `socket.connect` with arguments `self`, `address`.

`socket.``detach`()

  Put the socket object into closed state without actually closing the underlying file descriptor. The file descriptor is returned, and can be reused for other purposes.

  3.2 新版功能.

`socket.``dup`()

  Duplicate the socket.

  The newly created socket is non-inheritable.

  在 3.4 版更改: The socket is now non-inheritable.

`socket.``fileno`()

  Return the socket's file descriptor (a small integer), or -1 on failure. This is useful with `select.select()`.

  Under Windows the small integer returned by this method cannot be used where a file descriptor can be used (such as `os.fdopen()`). Unix does not have this limitation.

`socket.``get_inheritable`()

  Get the inheritable flag of the socket's file descriptor or socket's handle: `True` if the socket can be inherited in child processes, `False` if it cannot.

  3.4 新版功能.

`socket.``getpeername`()

  Return the remote address to which the socket is connected. This is useful to find out the port number of a remote IPv4/v6 socket, for instance. (The format of the address returned depends on the address family --- see above.) On some systems this function is not supported.

`socket.``getsockname`()

  Return the socket's own address. This is useful to find out the port number of an IPv4/v6 socket, for instance. (The format of the address returned depends on the address family --- see above.)

`socket.``getsockopt`(level, optname[, buflen])

  Return the value of the given socket option (see the Unix man page getsockopt(2)). The needed symbolic constants (`SO_*` etc.) are defined in this module. If buflen is absent, an integer option is assumed and its integer value is returned by the function. If buflen is present, it specifies the maximum length of the buffer used to receive the option in, and this buffer is returned as a bytes object. It is up to the caller to decode the contents of the buffer (see the optional built-in module `struct` for a way to decode C structures encoded as byte strings).

`socket.``getblocking`()

  Return `True` if socket is in blocking mode, `False` if in non-blocking.

  This is equivalent to checking `socket.gettimeout() == 0`.

  3.7 新版功能.

`socket.``gettimeout`()

  Return the timeout in seconds (float) associated with socket operations, or `None` if no timeout is set. This reflects the last call to `setblocking()` or `settimeout()`.

`socket.``ioctl`(control, option)
  Platform

    Windows

  The `ioctl()` method is a limited interface to the WSAIoctl system interface. Please refer to the Win32 documentation for more information.

  On other platforms, the generic `fcntl.fcntl()` and `fcntl.ioctl()` functions may be used; they accept a socket object as their first argument.

  Currently only the following control codes are supported: `SIO_RCVALL`, `SIO_KEEPALIVE_VALS`, and `SIO_LOOPBACK_FAST_PATH`.

  在 3.6 版更改: `SIO_LOOPBACK_FAST_PATH` was added.

`socket.``listen`([backlog])

  Enable a server to accept connections. If backlog is specified, it must be at least 0 (if it is lower, it is set to 0); it specifies the number of unaccepted connections that the system will allow before refusing new connections. If not specified, a default reasonable value is chosen.

  在 3.5 版更改: The backlog parameter is now optional.

`socket.``makefile`(mode='r', buffering=None, *, encoding=None, errors=None, newline=None)

  Return a file object associated with the socket. The exact returned type depends on the arguments given to `makefile()`. These arguments are interpreted the same way as by the built-in `open()` function, except the only supported mode values are `'r'` (default), `'w'` and `'b'`.

  The socket must be in blocking mode; it can have a timeout, but the file object's internal buffer may end up in an inconsistent state if a timeout occurs.

  Closing the file object returned by `makefile()` won't close the original socket unless all other file objects have been closed and `socket.close()` has been called on the socket object.

  注解

  On Windows, the file-like object created by `makefile()` cannot be used where a file object with a file descriptor is expected, such as the stream arguments of `subprocess.Popen()`.

`socket.``recv`(bufsize[, flags])

  Receive data from the socket. The return value is a bytes object representing the data received. The maximum amount of data to be received at once is specified by bufsize. See the Unix manual page recv(2) for the meaning of the optional argument flags; it defaults to zero.

  注解

  For best match with hardware and network realities, the value of bufsize should be a relatively small power of 2, for example, 4096.

  在 3.5 版更改: If the system call is interrupted and the signal handler does not raise an exception, the method now retries the system call instead of raising an `InterruptedError` exception (see PEP 475 for the rationale).

`socket.``recvfrom`(bufsize[, flags])

  Receive data from the socket. The return value is a pair `(bytes, address)` where bytes is a bytes object representing the data received and address is the address of the socket sending the data. See the Unix manual page recv(2) for the meaning of the optional argument flags; it defaults to zero. (The format of address depends on the address family --- see above.)

  在 3.5 版更改: If the system call is interrupted and the signal handler does not raise an exception, the method now retries the system call instead of raising an `InterruptedError` exception (see PEP 475 for the rationale).

  在 3.7 版更改: For multicast IPv6 address, first item of address does not contain `%scope_id` part anymore. In order to get full IPv6 address use `getnameinfo()`.

`socket.``recvmsg`(bufsize[, ancbufsize[, flags]])

  Receive normal data (up to bufsize bytes) and ancillary data from the socket. The ancbufsize argument sets the size in bytes of the internal buffer used to receive the ancillary data; it defaults to 0, meaning that no ancillary data will be received. Appropriate buffer sizes for ancillary data can be calculated using `CMSG_SPACE()` or `CMSG_LEN()`, and items which do not fit into the buffer might be truncated or discarded. The flags argument defaults to 0 and has the same meaning as for `recv()`.

  The return value is a 4-tuple: `(data, ancdata, msg_flags, address)`. The data item is a `bytes` object holding the non-ancillary data received. The ancdata item is a list of zero or more tuples `(cmsg_level, cmsg_type, cmsg_data)` representing the ancillary data (control messages) received: cmsg_level and cmsg_type are integers specifying the protocol level and protocol-specific type respectively, and cmsg_data is a `bytes` object holding the associated data. The msg_flags item is the bitwise OR of various flags indicating conditions on the received message; see your system documentation for details. If the receiving socket is unconnected, address is the address of the sending socket, if available; otherwise, its value is unspecified.

  On some systems, `sendmsg()` and `recvmsg()` can be used to pass file descriptors between processes over an `AF_UNIX` socket. When this facility is used (it is often restricted to `SOCK_STREAM` sockets), `recvmsg()` will return, in its ancillary data, items of the form `(socket.SOL_SOCKET, socket.SCM_RIGHTS, fds)`, where fds is a `bytes` object representing the new file descriptors as a binary array of the native C `int` type. If `recvmsg()` raises an exception after the system call returns, it will first attempt to close any file descriptors received via this mechanism.

  Some systems do not indicate the truncated length of ancillary data items which have been only partially received. If an item appears to extend beyond the end of the buffer, `recvmsg()` will issue a `RuntimeWarning`, and will return the part of it which is inside the buffer provided it has not been truncated before the start of its associated data.

  On systems which support the `SCM_RIGHTS` mechanism, the following function will receive up to maxfds file descriptors, returning the message data and a list containing the descriptors (while ignoring unexpected conditions such as unrelated control messages being received). See also `sendmsg()`.

      import socket, array

      def recv_fds(sock, msglen, maxfds):
          fds = array.array("i")   # Array of ints
          msg, ancdata, flags, addr = sock.recvmsg(msglen, socket.CMSG_LEN(maxfds * fds.itemsize))
          for cmsg_level, cmsg_type, cmsg_data in ancdata:
              if cmsg_level == socket.SOL_SOCKET and cmsg_type == socket.SCM_RIGHTS:
                  # Append data, ignoring any truncated integers at the end.
                  fds.frombytes(cmsg_data[:len(cmsg_data) - (len(cmsg_data) % fds.itemsize)])
          return msg, list(fds)

  Availability: most Unix platforms, possibly others.

  3.3 新版功能.

  在 3.5 版更改: If the system call is interrupted and the signal handler does not raise an exception, the method now retries the system call instead of raising an `InterruptedError` exception (see PEP 475 for the rationale).

`socket.``recvmsg_into`(buffers[, ancbufsize[, flags]])

  Receive normal data and ancillary data from the socket, behaving as `recvmsg()` would, but scatter the non-ancillary data into a series of buffers instead of returning a new bytes object. The buffers argument must be an iterable of objects that export writable buffers (e.g. `bytearray` objects); these will be filled with successive chunks of the non-ancillary data until it has all been written or there are no more buffers. The operating system may set a limit (`sysconf()` value `SC_IOV_MAX`) on the number of buffers that can be used. The ancbufsize and flags arguments have the same meaning as for `recvmsg()`.

  The return value is a 4-tuple: `(nbytes, ancdata, msg_flags, address)`, where nbytes is the total number of bytes of non-ancillary data written into the buffers, and ancdata, msg_flags and address are the same as for `recvmsg()`.

  示例:

      >>> import socket
      >>> s1, s2 = socket.socketpair()
      >>> b1 = bytearray(b'----')
      >>> b2 = bytearray(b'0123456789')
      >>> b3 = bytearray(b'--------------')
      >>> s1.send(b'Mary had a little lamb')
      22
      >>> s2.recvmsg_into([b1, memoryview(b2)[2:9], b3])
      (22, [], 0, None)
      >>> [b1, b2, b3]
      [bytearray(b'Mary'), bytearray(b'01 had a 9'), bytearray(b'little lamb---')]

  Availability: most Unix platforms, possibly others.

  3.3 新版功能.

`socket.``recvfrom_into`(buffer[, nbytes[, flags]])

  Receive data from the socket, writing it into buffer instead of creating a new bytestring. The return value is a pair `(nbytes, address)` where nbytes is the number of bytes received and address is the address of the socket sending the data. See the Unix manual page recv(2) for the meaning of the optional argument flags; it defaults to zero. (The format of address depends on the address family --- see above.)

`socket.``recv_into`(buffer[, nbytes[, flags]])

  Receive up to nbytes bytes from the socket, storing the data into a buffer rather than creating a new bytestring. If nbytes is not specified (or 0), receive up to the size available in the given buffer. Returns the number of bytes received. See the Unix manual page recv(2) for the meaning of the optional argument flags; it defaults to zero.

`socket.``send`(bytes[, flags])

  Send data to the socket. The socket must be connected to a remote socket. The optional flags argument has the same meaning as for `recv()` above. Returns the number of bytes sent. Applications are responsible for checking that all data has been sent; if only some of the data was transmitted, the application needs to attempt delivery of the remaining data. For further information on this topic, consult the 套接字编程指南.

  在 3.5 版更改: If the system call is interrupted and the signal handler does not raise an exception, the method now retries the system call instead of raising an `InterruptedError` exception (see PEP 475 for the rationale).

`socket.``sendall`(bytes[, flags])

  Send data to the socket. The socket must be connected to a remote socket. The optional flags argument has the same meaning as for `recv()` above. Unlike `send()`, this method continues to send data from bytes until either all data has been sent or an error occurs. `None` is returned on success. On error, an exception is raised, and there is no way to determine how much data, if any, was successfully sent.

  在 3.5 版更改: The socket timeout is no more reset each time data is sent successfully. The socket timeout is now the maximum total duration to send all data.

  在 3.5 版更改: If the system call is interrupted and the signal handler does not raise an exception, the method now retries the system call instead of raising an `InterruptedError` exception (see PEP 475 for the rationale).

`socket.``sendto`(bytes, address)
`socket.``sendto`(bytes, flags, address)

  Send data to the socket. The socket should not be connected to a remote socket, since the destination socket is specified by address. The optional flags argument has the same meaning as for `recv()` above. Return the number of bytes sent. (The format of address depends on the address family --- see above.)

  Raises an auditing event `socket.sendto` with arguments `self`, `address`.

  在 3.5 版更改: If the system call is interrupted and the signal handler does not raise an exception, the method now retries the system call instead of raising an `InterruptedError` exception (see PEP 475 for the rationale).

`socket.``sendmsg`(buffers[, ancdata[, flags[, address]]])

  Send normal and ancillary data to the socket, gathering the non-ancillary data from a series of buffers and concatenating it into a single message. The buffers argument specifies the non-ancillary data as an iterable of bytes-like objects (e.g. `bytes` objects); the operating system may set a limit (`sysconf()` value `SC_IOV_MAX`) on the number of buffers that can be used. The ancdata argument specifies the ancillary data (control messages) as an iterable of zero or more tuples `(cmsg_level, cmsg_type, cmsg_data)`, where cmsg_level and cmsg_type are integers specifying the protocol level and protocol-specific type respectively, and cmsg_data is a bytes-like object holding the associated data. Note that some systems (in particular, systems without `CMSG_SPACE()`) might support sending only one control message per call. The flags argument defaults to 0 and has the same meaning as for `send()`. If address is supplied and not `None`, it sets a destination address for the message. The return value is the number of bytes of non-ancillary data sent.

  The following function sends the list of file descriptors fds over an `AF_UNIX` socket, on systems which support the `SCM_RIGHTS` mechanism. See also `recvmsg()`.

      import socket, array

      def send_fds(sock, msg, fds):
          return sock.sendmsg([msg], [(socket.SOL_SOCKET, socket.SCM_RIGHTS, array.array("i", fds))])

  Availability: most Unix platforms, possibly others.

  Raises an auditing event `socket.sendmsg` with arguments `self`, `address`.

  3.3 新版功能.

  在 3.5 版更改: If the system call is interrupted and the signal handler does not raise an exception, the method now retries the system call instead of raising an `InterruptedError` exception (see PEP 475 for the rationale).

`socket.``sendmsg_afalg`([msg, ]*, op[, iv[, assoclen[, flags]]])

  Specialized version of `sendmsg()` for `AF_ALG` socket. Set mode, IV, AEAD associated data length and flags for `AF_ALG` socket.

  Availability: Linux >= 2.6.38.

  3.6 新版功能.

`socket.``send_fds`(sock, buffers, fds[, flags[, address]])

  Send the list of file descriptors fds over an `AF_UNIX` socket. The fds parameter is a sequence of file descriptors. Consult `sendmsg()` for the documentation of these parameters.

  Availability: Unix supporting `sendmsg()` and `SCM_RIGHTS` mechanism.

  3.9 新版功能.

`socket.``recv_fds`(sock, bufsize, maxfds[, flags])

  Receive up to maxfds file descriptors. Return `(msg, list(fds), flags, addr)`. Consult `recvmsg()` for the documentation of these parameters.

  Availability: Unix supporting `recvmsg()` and `SCM_RIGHTS` mechanism.

  3.9 新版功能.

  注解

  Any truncated integers at the end of the list of file descriptors.

`socket.``sendfile`(file, offset=0, count=None)

  Send a file until EOF is reached by using high-performance `os.sendfile` and return the total number of bytes which were sent. file must be a regular file object opened in binary mode. If `os.sendfile` is not available (e.g. Windows) or file is not a regular file `send()` will be used instead. offset tells from where to start reading the file. If specified, count is the total number of bytes to transmit as opposed to sending the file until EOF is reached. File position is updated on return or also in case of error in which case `file.tell()` can be used to figure out the number of bytes which were sent. The socket must be of `SOCK_STREAM` type. Non-blocking sockets are not supported.

  3.5 新版功能.

`socket.``set_inheritable`(inheritable)

  Set the inheritable flag of the socket's file descriptor or socket's handle.

  3.4 新版功能.

`socket.``setblocking`(flag)

  Set blocking or non-blocking mode of the socket: if flag is false, the socket is set to non-blocking, else to blocking mode.

  This method is a shorthand for certain `settimeout()` calls:

  - `sock.setblocking(True)` is equivalent to `sock.settimeout(None)`

  - `sock.setblocking(False)` is equivalent to `sock.settimeout(0.0)`

  在 3.7 版更改: The method no longer applies `SOCK_NONBLOCK` flag on `socket.type`.

`socket.``settimeout`(value)

  Set a timeout on blocking socket operations. The value argument can be a nonnegative floating point number expressing seconds, or `None`. If a non-zero value is given, subsequent socket operations will raise a `timeout` exception if the timeout period value has elapsed before the operation has completed. If zero is given, the socket is put in non-blocking mode. If `None` is given, the socket is put in blocking mode.

  For further information, please consult the notes on socket timeouts.

  在 3.7 版更改: The method no longer toggles `SOCK_NONBLOCK` flag on `socket.type`.

`socket.``setsockopt`(level, optname, value: int)

`socket.``setsockopt`(level, optname, value: buffer)

`socket.``setsockopt`(level, optname, None, optlen: int)

  Set the value of the given socket option (see the Unix manual page setsockopt(2)). The needed symbolic constants are defined in the `socket` module (`SO_*` etc.). The value can be an integer, `None` or a bytes-like object representing a buffer. In the later case it is up to the caller to ensure that the bytestring contains the proper bits (see the optional built-in module `struct` for a way to encode C structures as bytestrings). When value is set to `None`, optlen argument is required. It's equivalent to call `setsockopt()` C function with `optval=NULL` and `optlen=optlen`.

  在 3.5 版更改: 现在支持可写的 字节类对象。

  在 3.6 版更改: setsockopt(level, optname, None, optlen: int) form added.

`socket.``shutdown`(how)

  Shut down one or both halves of the connection. If how is `SHUT_RD`, further receives are disallowed. If how is `SHUT_WR`, further sends are disallowed. If how is `SHUT_RDWR`, further sends and receives are disallowed.

`socket.``share`(process_id)

  Duplicate a socket and prepare it for sharing with a target process. The target process must be provided with process_id. The resulting bytes object can then be passed to the target process using some form of interprocess communication and the socket can be recreated there using `fromshare()`. Once this method has been called, it is safe to close the socket since the operating system has already duplicated it for the target process.

  可用性: Windows。

  3.3 新版功能.

Note that there are no methods `read()` or `write()`; use `recv()` and `send()` without flags argument instead.

Socket objects also have these (read-only) attributes that correspond to the values given to the `socket` constructor.

`socket.``family`

  The socket family.

`socket.``type`

  The socket type.

`socket.``proto`

  The socket protocol.

## Notes on socket timeouts

A socket object can be in one of three modes: blocking, non-blocking, or timeout. Sockets are by default always created in blocking mode, but this can be changed by calling `setdefaulttimeout()`.

- In blocking mode, operations block until complete or the system returns an error (such as connection timed out).

- In non-blocking mode, operations fail (with an error that is unfortunately system-dependent) if they cannot be completed immediately: functions from the `select` can be used to know when and whether a socket is available for reading or writing.

- In timeout mode, operations fail if they cannot be completed within the timeout specified for the socket (they raise a `timeout` exception) or if the system returns an error.

注解

At the operating system level, sockets in timeout mode are internally set in non-blocking mode. Also, the blocking and timeout modes are shared between file descriptors and socket objects that refer to the same network endpoint. This implementation detail can have visible consequences if e.g. you decide to use the `fileno()` of a socket.

### Timeouts and the `connect` method

The `connect()` operation is also subject to the timeout setting, and in general it is recommended to call `settimeout()` before calling `connect()` or pass a timeout parameter to `create_connection()`. However, the system network stack may also return a connection timeout error of its own regardless of any Python socket timeout setting.

### Timeouts and the `accept` method

If `getdefaulttimeout()` is not `None`, sockets returned by the `accept()` method inherit that timeout. Otherwise, the behaviour depends on settings of the listening socket:

- if the listening socket is in blocking mode or in timeout mode, the socket returned by `accept()` is in blocking mode;

- if the listening socket is in non-blocking mode, whether the socket returned by `accept()` is in blocking or non-blocking mode is operating system-dependent. If you want to ensure cross-platform behaviour, it is recommended you manually override this setting.

## 示例

Here are four minimal example programs using the TCP/IP protocol: a server that echoes all data that it receives back (servicing only one client), and a client using it. Note that a server must perform the sequence `socket()`, `bind()`, `listen()`, `accept()` (possibly repeating the `accept()` to service more than one client), while a client only needs the sequence `socket()`, `connect()`. Also note that the server does not `sendall()`/`recv()` on the socket it is listening on but on the new socket returned by `accept()`.

The first two examples support IPv4 only.

    # Echo server program
    import socket

    HOST = ''                 # Symbolic name meaning all available interfaces
    PORT = 50007              # Arbitrary non-privileged port
    with socket.socket(socket.AF_INET, socket.SOCK_STREAM) as s:
        s.bind((HOST, PORT))
        s.listen(1)
        conn, addr = s.accept()
        with conn:
            print('Connected by', addr)
            while True:
                data = conn.recv(1024)
                if not data: break
                conn.sendall(data)

    # Echo client program
    import socket

    HOST = 'daring.cwi.nl'    # The remote host
    PORT = 50007              # The same port as used by the server
    with socket.socket(socket.AF_INET, socket.SOCK_STREAM) as s:
        s.connect((HOST, PORT))
        s.sendall(b'Hello, world')
        data = s.recv(1024)
    print('Received', repr(data))

The next two examples are identical to the above two, but support both IPv4 and IPv6. The server side will listen to the first address family available (it should listen to both instead). On most of IPv6-ready systems, IPv6 will take precedence and the server may not accept IPv4 traffic. The client side will try to connect to the all addresses returned as a result of the name resolution, and sends traffic to the first one connected successfully.

    # Echo server program
    import socket
    import sys

    HOST = None               # Symbolic name meaning all available interfaces
    PORT = 50007              # Arbitrary non-privileged port
    s = None
    for res in socket.getaddrinfo(HOST, PORT, socket.AF_UNSPEC,
                                  socket.SOCK_STREAM, 0, socket.AI_PASSIVE):
        af, socktype, proto, canonname, sa = res
        try:
            s = socket.socket(af, socktype, proto)
        except OSError as msg:
            s = None
            continue
        try:
            s.bind(sa)
            s.listen(1)
        except OSError as msg:
            s.close()
            s = None
            continue
        break
    if s is None:
        print('could not open socket')
        sys.exit(1)
    conn, addr = s.accept()
    with conn:
        print('Connected by', addr)
        while True:
            data = conn.recv(1024)
            if not data: break
            conn.send(data)

    # Echo client program
    import socket
    import sys

    HOST = 'daring.cwi.nl'    # The remote host
    PORT = 50007              # The same port as used by the server
    s = None
    for res in socket.getaddrinfo(HOST, PORT, socket.AF_UNSPEC, socket.SOCK_STREAM):
        af, socktype, proto, canonname, sa = res
        try:
            s = socket.socket(af, socktype, proto)
        except OSError as msg:
            s = None
            continue
        try:
            s.connect(sa)
        except OSError as msg:
            s.close()
            s = None
            continue
        break
    if s is None:
        print('could not open socket')
        sys.exit(1)
    with s:
        s.sendall(b'Hello, world')
        data = s.recv(1024)
    print('Received', repr(data))

The next example shows how to write a very simple network sniffer with raw sockets on Windows. The example requires administrator privileges to modify the interface:

    import socket

    # the public network interface
    HOST = socket.gethostbyname(socket.gethostname())

    # create a raw socket and bind it to the public interface
    s = socket.socket(socket.AF_INET, socket.SOCK_RAW, socket.IPPROTO_IP)
    s.bind((HOST, 0))

    # Include IP headers
    s.setsockopt(socket.IPPROTO_IP, socket.IP_HDRINCL, 1)

    # receive all packages
    s.ioctl(socket.SIO_RCVALL, socket.RCVALL_ON)

    # receive a package
    print(s.recvfrom(65565))

    # disabled promiscuous mode
    s.ioctl(socket.SIO_RCVALL, socket.RCVALL_OFF)

The next example shows how to use the socket interface to communicate to a CAN network using the raw socket protocol. To use CAN with the broadcast manager protocol instead, open a socket with:

    socket.socket(socket.AF_CAN, socket.SOCK_DGRAM, socket.CAN_BCM)

After binding (`CAN_RAW`) or connecting (`CAN_BCM`) the socket, you can use the `socket.send()`, and the `socket.recv()` operations (and their counterparts) on the socket object as usual.

This last example might require special privileges:

    import socket
    import struct

    # CAN frame packing/unpacking (see 'struct can_frame' in <linux/can.h>)

    can_frame_fmt = "=IB3x8s"
    can_frame_size = struct.calcsize(can_frame_fmt)

    def build_can_frame(can_id, data):
        can_dlc = len(data)
        data = data.ljust(8, b'\x00')
        return struct.pack(can_frame_fmt, can_id, can_dlc, data)

    def dissect_can_frame(frame):
        can_id, can_dlc, data = struct.unpack(can_frame_fmt, frame)
        return (can_id, can_dlc, data[:can_dlc])

    # create a raw socket and bind it to the 'vcan0' interface
    s = socket.socket(socket.AF_CAN, socket.SOCK_RAW, socket.CAN_RAW)
    s.bind(('vcan0',))

    while True:
        cf, addr = s.recvfrom(can_frame_size)

        print('Received: can_id=%x, can_dlc=%x, data=%s' % dissect_can_frame(cf))

        try:
            s.send(cf)
        except OSError:
            print('Error sending CAN frame')

        try:
            s.send(build_can_frame(0x01, b'\x01\x02\x03'))
        except OSError:
            print('Error sending CAN frame')

Running an example several times with too small delay between executions, could lead to this error:

    OSError: [Errno 98] Address already in use

This is because the previous execution has left the socket in a `TIME_WAIT` state, and can't be immediately reused.

There is a `socket` flag to set, in order to prevent this, `socket.SO_REUSEADDR`:

    s = socket.socket(socket.AF_INET, socket.SOCK_STREAM)
    s.setsockopt(socket.SOL_SOCKET, socket.SO_REUSEADDR, 1)
    s.bind((HOST, PORT))

the `SO_REUSEADDR` flag tells the kernel to reuse a local socket in `TIME_WAIT` state, without waiting for its natural timeout to expire.

参见

For an introduction to socket programming (in C), see the following papers:

- An Introductory 4.3BSD Interprocess Communication Tutorial, by Stuart Sechrest

- An Advanced 4.3BSD Interprocess Communication Tutorial, by Samuel J. Leffler et al,

both in the UNIX Programmer's Manual, Supplementary Documents 1 (sections PS1:7 and PS1:8). The platform-specific reference material for the various socket-related system calls are also a valuable source of information on the details of socket semantics. For Unix, refer to the manual pages; for Windows, see the WinSock (or Winsock 2) specification. For IPv6-ready APIs, readers may want to refer to RFC 3493 titled Basic Socket Interface Extensions for IPv6.