# `socket` --- 底层网络接口

源代码: Lib/socket.py

这个模块提供了访问 BSD 套接字 的接口。在所有现代 Unix 系统、Windows、macOS 和其他一些平台上可用。

注解

一些行为可能因平台不同而异，因为调用的是操作系统的套接字API。

这个Python接口是用Python的面向对象风格对Unix系统调用和套接字库接口的直译：函数 `socket()` 返回一个 套接字对象 ，其方法是对各种套接字系统调用的实现。形参类型一般与C接口相比更高级：例如在Python文件 `read()` 和 `write()` 操作中，接收操作的缓冲区分配是自动的，发送操作的缓冲区长度是隐式的。

参见

模块 `socketserver`

  用于简化网络服务端编写的类。

模块 `ssl`

  套接字对象的TLS/SSL封装。

## 套接字协议族

根据系统以及构建选项，此模块提供了各种套接字协议簇。

特定的套接字对象需要的地址格式将根据此套接字对象被创建时指定的地址族被自动选择。套接字地址表示如下：

- 一个绑定在文件系统节点上的 `AF_UNIX` 套接字的地址表示为一个字符串，使用文件系统字符编码和 `'surrogateescape'` 错误回调方法（see PEP 383）。一个地址在 Linux 的抽象命名空间被返回为带有初始的 null 字节的 字节类对象 ；注意在这个命名空间种的套接字可能与普通文件系统套接字通信，所以打算运行在 Linux 上的程序可能需要解决两种地址类型。当传递为参数时，一个字符串或字节类对象可以用于任一类型的地址。

  > 在 3.3 版更改: 之前，`AF_UNIX` 套接字路径被假设使用 UTF-8 编码。

  > 在 3.5 版更改: 现在支持可写的 字节类对象。

- 一对 `(host, port)` 被用于 `AF_INET` 地址族，host 是一个表示为互联网域名表示法之内的主机名或者一个 IPv4 地址的字符串，例如 `'daring.cwi.nl'` 或 `'100.50.200.5'`，port 是一个整数。

  - 对于 IPv4 地址，有两种可接受的特殊形式被用来代替一个主机地址： `''` 代表 `INADDR_ANY`，用来绑定到所有接口；字符串 `'<broadcast>'` 代表 `INADDR_BROADCAST`。此行为不兼容 IPv6，因此，如果你的 Python 程序打算支持 IPv6，则可能需要避开这些。

- For `AF_INET6` address family, a four-tuple `(host, port, flowinfo, scope_id)` is used, where flowinfo and scope_id represent the `sin6_flowinfo` and `sin6_scope_id` members in `struct sockaddr_in6` in C. For `socket` module methods, flowinfo and scope_id can be omitted just for backward compatibility. Note, however, omission of scope_id can cause problems in manipulating scoped IPv6 addresses.

  在 3.7 版更改: For multicast addresses (with scope_id meaningful) address may not contain `%scope_id` (or `zone id`) part. This information is superfluous and may be safely omitted (recommended).

- `AF_NETLINK` 套接字由一对 `(pid, groups)` 表示。

- 指定 `AF_TIPC` 地址族可以使用仅 Linux 支持的 TIPC 协议。TIPC 是一种开放的、非基于 IP 的网络协议，旨在用于集群计算环境。其地址用元组表示，其中的字段取决于地址类型。一般元组形式为 `(addr_type, v1, v2, v3 [, scope])`，其中：

  - addr_type 取 `TIPC_ADDR_NAMESEQ`、`TIPC_ADDR_NAME` 或 `TIPC_ADDR_ID` 中的一个。

  - scope 取 `TIPC_ZONE_SCOPE`、`TIPC_CLUSTER_SCOPE` 和 `TIPC_NODE_SCOPE` 中的一个。

  - 如果 addr_type 为 `TIPC_ADDR_NAME`，那么 v1 是服务器类型，v2 是端口标识符，v3 应为 0。

    如果 addr_type 为 `TIPC_ADDR_NAMESEQ`，那么 v1 是服务器类型，v2 是端口号下限，而 v3 是端口号上限。

    如果 addr_type 为 `TIPC_ADDR_ID`，那么 v1 是节点 (node)，v2 是 ref，v3 应为 0。

- `AF_CAN` 地址族使用元组 `(interface, )`，其中 interface 是表示网络接口名称的字符串，如 `'can0'`。网络接口名 `''` 可以用于接收本族所有网络接口的数据包。

  - `CAN_ISOTP` 协议接受一个元组 `(interface, rx_addr, tx_addr)`，其中两个额外参数都是无符号长整数，都表示 CAN 标识符（标准或扩展标识符）。

  - `CAN_J1939` protocol require a tuple `(interface, name, pgn, addr)` where additional parameters are 64-bit unsigned integer representing the ECU name, a 32-bit unsigned integer representing the Parameter Group Number (PGN), and an 8-bit integer representing the address.

- `PF_SYSTEM` 协议簇的 `SYSPROTO_CONTROL` 协议接受一个字符串或元组 `(id, unit)`。其中字符串是内核控件的名称，该控件使用动态分配的 ID。而如果 ID 和内核控件的单元 (unit) 编号都已知，或使用了已注册的 ID，可以采用元组。

  3.3 新版功能.

- `AF_BLUETOOTH` 支持以下协议和地址格式：

  - `BTPROTO_L2CAP` 接受 `(bdaddr, psm)`，其中 `bdaddr` 为字符串格式的蓝牙地址，`psm` 是一个整数。

  - `BTPROTO_RFCOMM` 接受 `(bdaddr, channel)`，其中 `bdaddr` 为字符串格式的蓝牙地址，`channel` 是一个整数。

  - `BTPROTO_HCI` 接受 `(device_id,)`，其中 `device_id` 为整数或字符串，它表示接口对应的蓝牙地址（具体取决于你的系统，NetBSD 和 DragonFlyBSD 需要蓝牙地址字符串，其他系统需要整数）。

    在 3.2 版更改: 添加了对 NetBSD 和 DragonFlyBSD 的支持。

  - `BTPROTO_SCO` 接受 `bdaddr`，其中 `bdaddr` 是 `bytes` 对象，其中含有字符串格式的蓝牙地址（如 `b'12:23:34:45:56:67'` ），FreeBSD 不支持此协议。

- `AF_ALG` 是一个仅 Linux 可用的、基于套接字的接口，用于连接内核加密算法。算法套接字可用包括 2 至 4 个元素的元组来配置 `(type, name [, feat [, mask]])`，其中：

  - type 是表示算法类型的字符串，如 `aead`、`hash`、`skcipher` 或 `rng`。

  - name 是表示算法类型和操作模式的字符串，如 `sha256`、`hmac(sha256)`、`cbc(aes)` 或 `drbg_nopr_ctr_aes256`。

  - feat 和 mask 是无符号 32 位整数。

  Availability: Linux 2.6.38, some algorithm types require more recent Kernels.

  3.6 新版功能.

- `AF_VSOCK` 用于支持虚拟机与宿主机之间的通讯。该套接字用 `(CID, port)` 元组表示，其中 Context ID (CID) 和 port 都是整数。

  Availability: Linux >= 4.8 QEMU >= 2.8 ESX >= 4.0 ESX Workstation >= 6.5.

  3.7 新版功能.

- `AF_PACKET` 是一个底层接口，直接连接至网卡。数据包使用元组 `(ifname, proto[, pkttype[, hatype[, addr]]])` 表示，其中：

  - ifname - 指定设备名称的字符串。

  - proto - 一个用网络字节序表示的整数，指定以太网协议版本号。

  - pkttype - 指定数据包类型的整数（可选）：

    - `PACKET_HOST` （默认） - 寻址到本地主机的数据包。

    - `PACKET_BROADCAST` - 物理层广播的数据包。

    - `PACKET_MULTIHOST` - 发送到物理层多播地址的数据包。

    - `PACKET_OTHERHOST` - 被（处于混杂模式的）网卡驱动捕获的、发送到其他主机的数据包。

    - `PACKET_OUTGOING` - 来自本地主机的、回环到一个套接字的数据包。

  - hatype - 可选整数，指定 ARP 硬件地址类型。

  - addr - 可选的类字节串对象，用于指定硬件物理地址，其解释取决于各设备。

- `AF_QIPCRTR` 是一个仅 Linux 可用的、基于套接字的接口，用于与高通平台中协处理器上运行的服务进行通信。该地址簇用一个 `(node, port)` 元组表示，其中 node 和 port 为非负整数。

  3.8 新版功能.

- `IPPROTO_UDPLITE` is a variant of UDP which allows you to specify what portion of a packet is covered with the checksum. It adds two socket options that you can change. `self.setsockopt(IPPROTO_UDPLITE, UDPLITE_SEND_CSCOV, length)` will change what portion of outgoing packets are covered by the checksum and `self.setsockopt(IPPROTO_UDPLITE, UDPLITE_RECV_CSCOV, length)` will filter out packets which cover too little of their data. In both cases `length` should be in `range(8, 2**16, 8)`.

  Such a socket should be constructed with `socket(AF_INET, SOCK_DGRAM, IPPROTO_UDPLITE)` for IPv4 or `socket(AF_INET6, SOCK_DGRAM, IPPROTO_UDPLITE)` for IPv6.

  Availability: Linux >= 2.6.20, FreeBSD >= 10.1-RELEASE

  3.9 新版功能.

如果你在 IPv4/v6 套接字地址的 host 部分中使用了一个主机名，此程序可能会表现不确定行为，因为 Python 使用 DNS 解析返回的第一个地址。套接字地址在实际的 IPv4/v6 中以不同方式解析，根据 DNS 解析和/或 host 配置。为了确定行为，在 host 部分中使用数字的地址。

所有的错误都抛出异常。对于无效的参数类型和内存溢出异常情况可能抛出普通异常；从 Python 3.3 开始，与套接字或地址语义有关的错误抛出 `OSError` 或它的子类之一（常用 `socket.error`）。

可以用 `setblocking()` 设置非阻塞模式。一个基于超时的 generalization 通过 `settimeout()` 支持。

## 模块内容

`socket` 模块导出以下元素。

### 异常

exception `socket.``error`

  一个被弃用的 `OSError` 的别名。

  在 3.3 版更改: 根据 PEP 3151，这个类是 `OSError` 的别名。

exception `socket.``herror`

  `OSError` 的子类，本异常通常表示与地址相关的错误，比如那些在 POSIX C API 中使用了 h_errno 的函数，包括 `gethostbyname_ex()` 和 `gethostbyaddr()`。附带的值是一对 `(h_errno, string)`，代表库调用返回的错误。h_errno 是一个数字，而 string 表示 h_errno 的描述，它们由 C 函数 `hstrerror()` 返回。

  在 3.3 版更改: 此类是 `OSError` 的子类。

exception `socket.``gaierror`

  `OSError` 的子类，本异常来自 `getaddrinfo()` 和 `getnameinfo()`，表示与地址相关的错误。附带的值是一对 `(error, string)`，代表库调用返回的错误。string 表示 error 的描述，它由 C 函数 `gai_strerror()` 返回。数字值 error 与本模块中定义的 `EAI_*` 常量之一匹配。

  在 3.3 版更改: 此类是 `OSError` 的子类。

exception `socket.``timeout`

  `OSError` 的子类，当套接字发生超时，且事先已调用过 `settimeout()` （或隐式地通过 `setdefaulttimeout()` ）启用了超时，则会抛出此异常。附带的值是一个字符串，其值总是 "timed out"。

  在 3.3 版更改: 此类是 `OSError` 的子类。

### 常数

> AF_* 和 SOCK_* 常量现在都在 `AddressFamily` 和 `SocketKind` 这两个 `IntEnum` 集合内。

> 3.4 新版功能.

`socket.``AF_UNIX`
`socket.``AF_INET`
`socket.``AF_INET6`

  这些常量表示地址（和协议）簇，用于 `socket()` 的第一个参数。如果 `AF_UNIX` 常量未定义，即表示不支持该协议。不同系统可能会有更多其他常量可用。

`socket.``SOCK_STREAM`
`socket.``SOCK_DGRAM`
`socket.``SOCK_RAW`
`socket.``SOCK_RDM`
`socket.``SOCK_SEQPACKET`

  这些常量表示套接字类型，用于 `socket()` 的第二个参数。不同系统可能会有更多其他常量可用。（一般只有 `SOCK_STREAM` 和 `SOCK_DGRAM` 可用）

`socket.``SOCK_CLOEXEC`
`socket.``SOCK_NONBLOCK`

  这两个常量（如果已定义）可以与上述套接字类型结合使用，允许你设置这些原子性相关的 flags （从而避免可能的竞争条件和单独调用的需要）。

  参见

  Secure File Descriptor Handling （安全地处理文件描述符） 提供了更详尽的解释。

  可用性： Linux >= 2.6.27。

  3.2 新版功能.

`SO_*`
`socket.``SOMAXCONN`
`MSG_*`
`SOL_*`
`SCM_*`
`IPPROTO_*`
`IPPORT_*`
`INADDR_*`
`IP_*`
`IPV6_*`
`EAI_*`
`AI_*`
`NI_*`
`TCP_*`

  此列表内的许多常量，记载在 Unix 文档中的套接字和/或 IP 协议部分，同时也定义在本 socket 模块中。它们通常用于套接字对象的 `setsockopt()` 和 `getsockopt()` 方法的参数中。在大多数情况下，仅那些在 Unix 头文件中有定义的符号会在本模块中定义，部分符号提供了默认值。

  在 3.6 版更改: 添加了 `SO_DOMAIN`、`SO_PROTOCOL`、`SO_PEERSEC`、`SO_PASSSEC`、`TCP_USER_TIMEOUT`、`TCP_CONGESTION`。

  在 3.6.5 版更改: 在 Windows 上，如果 Windows 运行时支持，则 `TCP_FASTOPEN`、`TCP_KEEPCNT` 可用。

  在 3.7 版更改: 添加了 `TCP_NOTSENT_LOWAT`。

  在 Windows 上，如果 Windows 运行时支持，则 `TCP_KEEPIDLE`、`TCP_KEEPINTVL` 可用。

`socket.``AF_CAN`
`socket.``PF_CAN`
`SOL_CAN_*`
`CAN_*`

  此列表内的许多常量，记载在 Linux 文档中，同时也定义在本 socket 模块中。

  可用性： Linux >= 2.6.25。

  3.3 新版功能.

`socket.``CAN_BCM`
`CAN_BCM_*`

  CAN 协议簇内的 CAN_BCM 是广播管理器（Bbroadcast Manager -- BCM）协议，广播管理器常量在 Linux 文档中有所记载，在本 socket 模块中也有定义。

  可用性： Linux >= 2.6.25。

  注解

  `CAN_BCM_CAN_FD_FRAME` 旗标仅在 Linux >= 4.8 时可用。

  3.4 新版功能.

`socket.``CAN_RAW_FD_FRAMES`

  在 CAN_RAW 套接字中启用 CAN FD 支持，默认是禁用的。它使应用程序可以发送 CAN 和 CAN FD 帧。但是，从套接字读取时，也必须同时接受 CAN 和 CAN FD 帧。

  此常量在 Linux 文档中有所记载。

  可用性： Linux >= 3.6。

  3.5 新版功能.

`socket.``CAN_RAW_JOIN_FILTERS`

  Joins the applied CAN filters such that only CAN frames that match all given CAN filters are passed to user space.

  此常量在 Linux 文档中有所记载。

  Availability: Linux >= 4.1.

  3.9 新版功能.

`socket.``CAN_ISOTP`

  CAN 协议簇中的 CAN_ISOTP 就是 ISO-TP (ISO 15765-2) 协议。ISO-TP 常量在 Linux 文档中有所记载。

  可用性： Linux >= 2.6.25。

  3.7 新版功能.

`socket.``CAN_J1939`

  CAN_J1939, in the CAN protocol family, is the SAE J1939 protocol. J1939 constants, documented in the Linux documentation.

  Availability: Linux >= 5.4.

  3.9 新版功能.

`socket.``AF_PACKET`
`socket.``PF_PACKET`
`PACKET_*`

  此列表内的许多常量，记载在 Linux 文档中，同时也定义在本 socket 模块中。

  可用性： Linux >= 2.2。

`socket.``AF_RDS`
`socket.``PF_RDS`
`socket.``SOL_RDS`
`RDS_*`

  此列表内的许多常量，记载在 Linux 文档中，同时也定义在本 socket 模块中。

  可用性： Linux >= 2.6.30。

  3.3 新版功能.

`socket.``SIO_RCVALL`
`socket.``SIO_KEEPALIVE_VALS`
`socket.``SIO_LOOPBACK_FAST_PATH`
`RCVALL_*`

  Windows 的 WSAIoctl() 的常量。这些常量用于套接字对象的 `ioctl()` 方法的参数。

  在 3.6 版更改: 添加了 `SIO_LOOPBACK_FAST_PATH`。

`TIPC_*`

  TIPC 相关常量，与 C socket API 导出的常量一致。更多信息请参阅 TIPC 文档。

`socket.``AF_ALG`
`socket.``SOL_ALG`
`ALG_*`

  用于 Linux 内核加密算法的常量。

  可用性： Linux >= 2.6.38。

  3.6 新版功能.

`socket.``AF_VSOCK`
`socket.``IOCTL_VM_SOCKETS_GET_LOCAL_CID`
`VMADDR*`
`SO_VM*`

  用于 Linux 宿主机/虚拟机通讯的常量。

  可用性： Linux >= 4.8。

  3.7 新版功能.

`socket.``AF_LINK`

  可用性： BSD、OSX。

  3.4 新版功能.

`socket.``has_ipv6`

  本常量为一个布尔值，该值指示当前平台是否支持 IPv6。

`socket.``BDADDR_ANY`
`socket.``BDADDR_LOCAL`

  这些是字符串常量，包含蓝牙地址，这些地址具有特殊含义。例如，当用 `BTPROTO_RFCOMM` 指定绑定套接字时， `BDADDR_ANY` 表示“任何地址”。

`socket.``HCI_FILTER`
`socket.``HCI_TIME_STAMP`
`socket.``HCI_DATA_DIR`

  与 `BTPROTO_HCI` 一起使用。 `HCI_FILTER` 在 NetBSD 或 DragonFlyBSD 上不可用。 `HCI_TIME_STAMP` 和 `HCI_DATA_DIR` 在 FreeBSD、NetBSD 或 DragonFlyBSD 上不可用。

`socket.``AF_QIPCRTR`

  高通 IPC 路由协议的常数，用于与提供远程处理器的服务进行通信。

  可用性： Linux >= 4.7。

### 函数

#### 创建套接字

下列函数都能创建 套接字对象.

`socket.``socket`(family=AF_INET, type=SOCK_STREAM, proto=0, fileno=None)

  Create a new socket using the given address family, socket type and protocol number. The address family should be `AF_INET` (the default), `AF_INET6`, `AF_UNIX`, `AF_CAN`, `AF_PACKET`, or `AF_RDS`. The socket type should be `SOCK_STREAM` (the default), `SOCK_DGRAM`, `SOCK_RAW` or perhaps one of the other `SOCK_` constants. The protocol number is usually zero and may be omitted or in the case where the address family is `AF_CAN` the protocol should be one of `CAN_RAW`, `CAN_BCM`, `CAN_ISOTP` or `CAN_J1939`.

  如果指定了 fileno，那么将从这一指定的文件描述符中自动检测 family、type 和 proto 的值。如果调用本函数时显式指定了 family、type 或 proto 参数，可以覆盖自动检测的值。这只会影响 Python 表示诸如 `socket.getpeername()` 一类函数的返回值的方式，而不影响实际的操作系统资源。与 `socket.fromfd()` 不同，fileno 将返回原先的套接字，而不是复制出新的套接字。这有助于在分离的套接字上调用 `socket.close()` 来关闭它。

  新创建的套接字是 不可继承的。

  引发一个 审计事件 `socket.__new__` 附带参数 `self`、`family`、`type`、`protocol`。

  在 3.3 版更改: 添加了 AF_CAN 簇。添加了 AF_RDS 簇。

  在 3.4 版更改: 添加了 CAN_BCM 协议。

  在 3.4 版更改: 返回的套接字现在是不可继承的。

  在 3.7 版更改: 添加了 CAN_ISOTP 协议。

  在 3.7 版更改: 当将 `SOCK_NONBLOCK` 或 `SOCK_CLOEXEC` 标志位应用于 type 上时，它们会被清除，且 `socket.type` 反映不出它们。但它们仍将传递给底层系统的 socket() 调用。因此，

      sock = socket.socket(
          socket.AF_INET,
          socket.SOCK_STREAM | socket.SOCK_NONBLOCK)

  仍将在支持 `SOCK_NONBLOCK` 的系统上创建一个非阻塞的套接字，但是 `sock.type` 会被置为 `socket.SOCK_STREAM`。

  在 3.9 版更改: The CAN_J1939 protocol was added.

`socket.``socketpair`([family[, type[, proto]]])

  构建一对已连接的套接字对象，使用给定的地址簇、套接字类型和协议号。地址簇、套接字类型和协议号与上述 `socket()` 函数相同。默认地址簇为 `AF_UNIX` （需要当前平台支持，不支持则默认为 `AF_INET` ）。

  新创建的套接字都是 不可继承的。

  在 3.2 版更改: 现在，返回的套接字对象支持全部套接字 API，而不是全部 API 的一个子集。

  在 3.4 版更改: 返回的套接字现在都是不可继承的。

  在 3.5 版更改: 添加了 Windows 支持。

`socket.``create_connection`(address[, timeout[, source_address]])

  连接到一个 TCP 服务，该服务正在侦听 Internet address （用二元组 `(host, port)` 表示）。连接后返回套接字对象。这是比 `socket.connect()` 更高级的函数：如果 host 是非数字主机名，它将尝试从 `AF_INET` 和 `AF_INET6` 解析它，然后依次尝试连接到所有可能的地址，直到连接成功。这使得编写兼容 IPv4 和 IPv6 的客户端变得容易。

  传入可选参数 timeout 可以在套接字实例上设置超时（在尝试连接前）。如果未提供 timeout，则使用由 `getdefaulttimeout()` 返回的全局默认超时设置。

  如果提供了 source_address，它必须为二元组 `(host, port)`，以便套接字在连接之前绑定为其源地址。如果 host 或 port 分别为 '' 或 0，则使用操作系统默认行为。

  在 3.2 版更改: 添加了 source_address。

`socket.``create_server`(address, *, family=AF_INET, backlog=None, reuse_port=False, dualstack_ipv6=False)

  便捷函数，创建绑定到 address （二元组 `(host, port)` ）的 TCP 套接字，返回套接字对象。

  family 应设置为 `AF_INET` 或 `AF_INET6`。backlog 是传递给 `socket.listen()` 的队列大小，当它为 `0` 则表示默认的合理值。reuse_port 表示是否设置 `SO_REUSEPORT` 套接字选项。

  如果 dualstack_ipv6 为 true 且平台支持，则套接字能接受 IPv4 和 IPv6 连接，否则将抛出 `ValueError` 异常。大多数 POSIX 平台和 Windows 应该支持此功能。启用此功能后，`socket.getpeername()` 在进行 IPv4 连接时返回的地址将是一个（映射到 IPv4 的）IPv6 地址。在默认启用该功能的平台上（如 Linux），如果 dualstack_ipv6 为 false，即显式禁用此功能。该参数可以与 `has_dualstack_ipv6()` 结合使用：

      import socket

      addr = ("", 8080)  # all interfaces, port 8080
      if socket.has_dualstack_ipv6():
          s = socket.create_server(addr, family=socket.AF_INET6, dualstack_ipv6=True)
      else:
          s = socket.create_server(addr)

  注解

  在 POSIX 平台上，设置 `SO_REUSEADDR` 套接字选项是为了立即重用以前绑定在同一 address 上并保持 TIME_WAIT 状态的套接字。

  3.8 新版功能.

`socket.``has_dualstack_ipv6`()

  如果平台支持创建 IPv4 和 IPv6 连接都可以处理的 TCP 套接字，则返回 `True`。

  3.8 新版功能.

`socket.``fromfd`(fd, family, type, proto=0)

  复制文件描述符 fd （一个由文件对象的 `fileno()` 方法返回的整数），然后从结果中构建一个套接字对象。地址簇、套接字类型和协议号与上述 `socket()` 函数相同。文件描述符应指向一个套接字，但不会专门去检查——如果文件描述符是无效的，则对该对象的后续操作可能会失败。本函数很少用到，但是在将套接字作为标准输入或输出传递给程序（如 Unix inet 守护程序启动的服务器）时，可以使用本函数获取或设置套接字选项。套接字将处于阻塞模式。

  新创建的套接字是 不可继承的。

  在 3.4 版更改: 返回的套接字现在是不可继承的。

`socket.``fromshare`(data)

  根据 `socket.share()` 方法获得的数据实例化套接字。套接字将处于阻塞模式。

  可用性: Windows。

  3.3 新版功能.

`socket.``SocketType`

  这是一个 Python 类型对象，表示套接字对象的类型。它等同于 `type(socket(...))`。

#### 其他功能

`socket` 模块还提供多种网络相关服务：

`socket.``close`(fd)

  关闭一个套接字文件描述符。它类似于 `os.close()`，但专用于套接字。在某些平台上（特别是在 Windows 上），`os.close()` 对套接字文件描述符无效。

  3.7 新版功能.

`socket.``getaddrinfo`(host, port, family=0, type=0, proto=0, flags=0)

  将 host/port 参数转换为 5 元组的序列，其中包含创建（连接到某服务的）套接字所需的所有参数。host 是域名，是字符串格式的 IPv4/v6 地址或 `None`。port 是字符串格式的服务名称，如 `'http'` 、端口号（数字）或 `None`。传入 `None` 作为 host 和 port 的值，相当于将 `NULL` 传递给底层 C API。

  可以指定 family、type 和 proto 参数，以缩小返回的地址列表。向这些参数分别传入 0 表示保留全部结果范围。flags 参数可以是 `AI_*` 常量中的一个或多个，它会影响结果的计算和返回。例如，`AI_NUMERICHOST` 会禁用域名解析，此时如果 host 是域名，则会抛出错误。

  本函数返回一个列表，其中的 5 元组具有以下结构：

  `(family, type, proto, canonname, sockaddr)`

  In these tuples, family, type, proto are all integers and are meant to be passed to the `socket()` function. canonname will be a string representing the canonical name of the host if `AI_CANONNAME` is part of the flags argument; else canonname will be empty. sockaddr is a tuple describing a socket address, whose format depends on the returned family (a `(address, port)` 2-tuple for `AF_INET`, a `(address, port, flowinfo, scope_id)` 4-tuple for `AF_INET6`), and is meant to be passed to the `socket.connect()` method.

  引发一个 审计事件 `socket.getaddrinfo` 附带参数 `host`、`port`、`family`、`type`、`protocol`。

  下面的示例获取了 TCP 连接地址信息，假设该连接通过 80 端口连接至 `example.org` （如果系统未启用 IPv6，则结果可能会不同）:

      >>> socket.getaddrinfo("example.org", 80, proto=socket.IPPROTO_TCP)
      [(<AddressFamily.AF_INET6: 10>, <SocketType.SOCK_STREAM: 1>,
       6, '', ('2606:2800:220:1:248:1893:25c8:1946', 80, 0, 0)),
       (<AddressFamily.AF_INET: 2>, <SocketType.SOCK_STREAM: 1>,
       6, '', ('93.184.216.34', 80))]

  在 3.2 版更改: 现在可以使用关键字参数的形式来传递参数。

  在 3.7 版更改: for IPv6 multicast addresses, string representing an address will not contain `%scope_id` part.

`socket.``getfqdn`([name])

  返回 name 的全限定域名 (Fully Qualified Domain Name -- FQDN)。如果 name 省略或为空，则将其解释为本地主机。为了查找全限定名称，首先将检查由 `gethostbyaddr()` 返回的主机名，然后是主机的别名（如果存在）。选中第一个包含句点的名字。如果无法获取全限定域名，则返回由 `gethostname()` 返回的主机名。

`socket.``gethostbyname`(hostname)

  将主机名转换为 IPv4 地址格式。IPv4 地址以字符串格式返回，如 `'100.50.200.5'`。如果主机名本身是 IPv4 地址，则原样返回。更完整的接口请参考 `gethostbyname_ex()`。 `gethostbyname()` 不支持 IPv6 名称解析，应使用 `getaddrinfo()` 来支持 IPv4/v6 双协议栈。

  引发一个 审计事件 `socket.gethostbyname`，附带参数 `hostname`。

`socket.``gethostbyname_ex`(hostname)

  将主机名转换为 IPv4 地址格式的扩展接口。返回三元组 `(hostname, aliaslist, ipaddrlist)`，其中 hostname 是响应给定 ip_address 的主要主机名，aliaslist 是相同地址的其他可用主机名的列表（可能为空），而 ipaddrlist 是 IPv4 地址列表，包含相同主机名、相同接口的不同地址（通常是一个地址，但不总是如此）。`gethostbyname_ex()` 不支持 IPv6 名称解析，应使用 `getaddrinfo()` 来支持 IPv4/v6 双协议栈。

  引发一个 审计事件 `socket.gethostbyname`，附带参数 `hostname`。

`socket.``gethostname`()

  返回一个字符串，包含当前正在运行 Python 解释器的机器的主机名。

  引发一个 审计事件 `socket.gethostname`，没有附带参数。

  注意： `gethostname()` 并不总是返回全限定域名，必要的话请使用 `getfqdn()`。

`socket.``gethostbyaddr`(ip_address)

  返回三元组 `(hostname, aliaslist, ipaddrlist)`，其中 hostname 是响应给定 ip_address 的主要主机名，aliaslist 是相同地址的其他可用主机名的列表（可能为空），而 ipaddrlist 是 IPv4/v6 地址列表，包含相同主机名、相同接口的不同地址（很可能仅包含一个地址）。要查询全限定域名，请使用函数 `getfqdn()`。`gethostbyaddr()` 支持 IPv4 和 IPv6。

  引发一个 审计事件 `socket.gethostbyaddr`，附带参数 `ip_address`。

`socket.``getnameinfo`(sockaddr, flags)

  将套接字地址 sockaddr 转换为二元组 `(host, port)`。host 的形式可能是全限定域名，或是由数字表示的地址，具体取决于 flags 的设置。同样，port 可以包含字符串格式的端口名称或数字格式的端口号。

  For IPv6 addresses, `%scope_id` is appended to the host part if sockaddr contains meaningful scope_id. Usually this happens for multicast addresses.

  关于 flags 的更多信息可参阅 getnameinfo(3)。

  引发一个 审计事件 `socket.getnameinfo`，附带参数 `sockaddr`。

`socket.``getprotobyname`(protocolname)

  将 Internet 协议名称（如 `'icmp'` ）转换为常量，该常量适用于 `socket()` 函数的第三个（可选）参数。通常只有在 "raw" 模式 (`SOCK_RAW`) 中打开的套接字才需要使用该常量。在正常的套接字模式下，协议省略或为零时，会自动选择正确的协议。

`socket.``getservbyname`(servicename[, protocolname])

  将 Internet 服务名称和协议名称转换为该服务的端口号。协议名称是可选的，如果提供的话应为 `'tcp'` 或 `'udp'`，否则将匹配出所有协议。

  引发一个 审计事件 `socket.getservbyname`，附带参数 `servicename`、`protocolname`。

`socket.``getservbyport`(port[, protocolname])

  将 Internet 端口号和协议名称转换为该服务的服务名称。协议名称是可选的，如果提供的话应为 `'tcp'` 或 `'udp'`，否则将匹配出所有协议。

  引发一个 审计事件 `socket.getservbyport`，附带参数 `port`、`protocolname`。

`socket.``ntohl`(x)

  将 32 位正整数从网络字节序转换为主机字节序。在主机字节序与网络字节序相同的计算机上，这是一个空操作。字节序不同将执行 4 字节交换操作。

`socket.``ntohs`(x)

  将 16 位正整数从网络字节序转换为主机字节序。在主机字节序与网络字节序相同的计算机上，这是一个空操作。字节序不同将执行 2 字节交换操作。

  3.7 版后已移除: 如果 x 不符合 16 位无符号整数，但符合 C 语言的正整数，则它会被静默截断为 16 位无符号整数。此静默截断功能已弃用，未来版本的 Python 将对此抛出异常。

`socket.``htonl`(x)

  将 32 位正整数从主机字节序转换为网络字节序。在主机字节序与网络字节序相同的计算机上，这是一个空操作。字节序不同将执行 4 字节交换操作。

`socket.``htons`(x)

  将 16 位正整数从主机字节序转换为网络字节序。在主机字节序与网络字节序相同的计算机上，这是一个空操作。字节序不同将执行 2 字节交换操作。

  3.7 版后已移除: 如果 x 不符合 16 位无符号整数，但符合 C 语言的正整数，则它会被静默截断为 16 位无符号整数。此静默截断功能已弃用，未来版本的 Python 将对此抛出异常。

`socket.``inet_aton`(ip_string)

  将 IPv4 地址从点分十进制字符串格式（如 '123.45.67.89' ）转换为 32 位压缩二进制格式，转换后为字节对象，长度为四个字符。与那些使用标准 C 库，且需要 `struct in_addr` 类型的对象的程序交换信息时，本函数很有用。 该类型即本函数返回的 32 位压缩二进制的 C 类型。

  `inet_aton()` 也接受句点数少于三的字符串，详情请参阅 Unix 手册 inet(3)。

  如果传入本函数的 IPv4 地址字符串无效，则抛出 `OSError`。注意，具体什么样的地址有效取决于 `inet_aton()` 的底层 C 实现。

  `inet_aton()` 不支持 IPv6，在 IPv4/v6 双协议栈下应使用 `inet_pton()` 来代替。

`socket.``inet_ntoa`(packed_ip)

  将 32 位压缩 IPv4 地址（一个 类字节对象，长 4 个字节）转换为标准的点分十进制字符串形式（如 '123.45.67.89' ）。与那些使用标准 C 库，且需要 `struct in_addr` 类型的对象的程序交换信息时，本函数很有用。 该类型即本函数参数中的 32 位压缩二进制数据的 C 类型。

  如果传入本函数的字节序列长度不是 4 个字节，则抛出 `OSError`。`inet_ntoa()` 不支持 IPv6，在 IPv4/v6 双协议栈下应使用 `inet_ntop()` 来代替。

  在 3.5 版更改: 现在支持可写的 字节类对象。

`socket.``inet_pton`(address_family, ip_string)

  将特定地址簇的 IP 地址（字符串）转换为压缩二进制格式。当库或网络协议需要接受 `struct in_addr` 类型的对象（类似 `inet_aton()` ）或 `struct in6_addr` 类型的对象时，`inet_pton()` 很有用。

  目前 address_family 支持 `AF_INET` 和 `AF_INET6`。如果 IP 地址字符串 ip_string 无效，则抛出 `OSError`。注意，具体什么地址有效取决于 address_family 的值和 `inet_pton()` 的底层实现。

  可用性： Unix（可能非所有平台都可用）、Windows。

  在 3.4 版更改: 添加了 Windows 支持

`socket.``inet_ntop`(address_family, packed_ip)

  将压缩 IP 地址（一个 类字节对象，数个字节长）转换为标准的、特定地址簇的字符串形式（如 `'7.10.0.5'` 或 `'5aef:2b::8'` ）。当库或网络协议返回 `struct in_addr` 类型的对象（类似 `inet_ntoa()` ）或 `struct in6_addr` 类型的对象时，`inet_ntop()` 很有用。

  目前 address_family 支持 `AF_INET` 和 `AF_INET6`。如果字节对象 packed_ip 与指定的地址簇长度不符，则抛出 `ValueError`。针对 `inet_ntop()` 调用的错误则抛出 `OSError`。

  可用性： Unix（可能非所有平台都可用）、Windows。

  在 3.4 版更改: 添加了 Windows 支持

  在 3.5 版更改: 现在支持可写的 字节类对象。

`socket.``CMSG_LEN`(length)

  返回给定 length 所关联数据的辅助数据项的总长度（不带尾部填充）。此值通常用作 `recvmsg()` 接收一个辅助数据项的缓冲区大小，但是 RFC 3542 要求可移植应用程序使用 `CMSG_SPACE()`，以此将尾部填充的空间计入，即使该项在缓冲区的最后。如果 length 超出允许范围，则抛出 `OverflowError`。

  可用性： 大多数 Unix 平台，其他平台也可能可用。

  3.3 新版功能.

`socket.``CMSG_SPACE`(length)

  返回 `recvmsg()` 所需的缓冲区大小，以接收给定 length 所关联数据的辅助数据项，带有尾部填充。接收多个项目所需的缓冲区空间是关联数据长度的 `CMSG_SPACE()` 值的总和。如果 length 超出允许范围，则抛出 `OverflowError`。

  请注意，某些系统可能支持辅助数据，但不提供本函数。还需注意，如果使用本函数的结果来设置缓冲区大小，可能无法精确限制可接收的辅助数据量，因为可能会有其他数据写入尾部填充区域。

  可用性： 大多数 Unix 平台，其他平台也可能可用。

  3.3 新版功能.

`socket.``getdefaulttimeout`()

  返回用于新套接字对象的默认超时（以秒为单位的浮点数）。值 `None` 表示新套接字对象没有超时。首次导入 socket 模块时，默认值为 `None`。

`socket.``setdefaulttimeout`(timeout)

  设置用于新套接字对象的默认超时（以秒为单位的浮点数）。首次导入 socket 模块时，默认值为 `None`。可能的取值及其各自的含义请参阅 `settimeout()`。

`socket.``sethostname`(name)

  将计算机的主机名设置为 name。如果权限不足将抛出 `OSError`。

  引发一个 审计事件 `socket.sethostname`，附带参数 `name`。

  Availability: Unix.

  3.3 新版功能.

`socket.``if_nameindex`()

  返回一个列表，包含网络接口（网卡）信息二元组（整数索引，名称字符串）。系统调用失败则抛出 `OSError`。

  可用性: Unix, Windows。

  3.3 新版功能.

  在 3.8 版更改: 添加了 Windows 支持。

`socket.``if_nametoindex`(if_name)

  返回网络接口名称相对应的索引号。如果没有所给名称的接口，则抛出 `OSError`。

  可用性: Unix, Windows。

  3.3 新版功能.

  在 3.8 版更改: 添加了 Windows 支持。

`socket.``if_indextoname`(if_index)

  返回网络接口索引号相对应的接口名称。如果没有所给索引号的接口，则抛出 `OSError`。

  可用性: Unix, Windows。

  3.3 新版功能.

  在 3.8 版更改: 添加了 Windows 支持。

## 套接字对象

套接字对象具有以下方法。除了 `makefile()`，其他都与套接字专用的 Unix 系统调用相对应。

在 3.2 版更改: 添加了对 上下文管理器 协议的支持。退出上下文管理器与调用 `close()` 等效。

`socket.``accept`()

  接受一个连接。此 scoket 必须绑定到一个地址上并且监听连接。返回值是一个 `(conn, address)` 对，其中 conn 是一个 新 的套接字对象，用于在此连接上收发数据，address 是连接另一端的套接字所绑定的地址。

  新创建的套接字是 不可继承的。

  在 3.4 版更改: 该套接字现在是不可继承的。

  在 3.5 版更改: 如果系统调用被中断，但信号处理程序没有触发异常，此方法现在会重试系统调用，而不是触发 `InterruptedError` 异常 (原因详见 PEP 475)。

`socket.``bind`(address)

  将套接字绑定到 address。套接字必须尚未绑定。（ address 的格式取决于地址簇 —— 参见上文）

  引发一个 审计事件 `socket.bind`，附带参数 `self`、`address`。

`socket.``close`()

  将套接字标记为关闭。当 `makefile()` 创建的所有文件对象都关闭时，底层系统资源（如文件描述符）也将关闭。一旦上述情况发生，将来对套接字对象的所有操作都会失败。对端将接收不到任何数据（清空队列数据后）。

  垃圾回收时，套接字会自动关闭，但建议显式 `close()` 它们，或在它们周围使用 `with` 语句。

  在 3.6 版更改: 现在，如果底层的 `close()` 调用出错，会抛出 `OSError`。

  注解

  `close()` 释放与连接相关联的资源，但不一定立即关闭连接。如果需要及时关闭连接，请在调用 `close()` 之前调用 `shutdown()`。

`socket.``connect`(address)

  连接到 address 处的远程套接字。（ address 的格式取决于地址簇 —— 参见上文）

  如果连接被信号中断，则本方法将等待，直到连接完成。如果信号处理程序未抛出异常，且套接字阻塞中或已超时，则在超时后抛出 `socket.timeout`。对于非阻塞套接字，如果连接被信号中断，则本方法将抛出 `InterruptedError` 异常（或信号处理程序抛出的异常）。

  引发一个 审计事件 `socket.connect`，附带参数 `self`、`address`。

  在 3.5 版更改: 本方法现在将等待，直到连接完成，而不是在以下情况抛出 `InterruptedError` 异常。该情况为，连接被信号中断，信号处理程序未抛出异常，且套接字阻塞中或已超时（具体解释请参阅 PEP 475 ）。

`socket.``connect_ex`(address)

  类似于 `connect(address)`，但是对于 C 级别的 `connect()` 调用返回的错误，本函数将返回错误指示器，而不是抛出异常（对于其他问题，如“找不到主机”，仍然可以抛出异常）。如果操作成功，则错误指示器为 `0`，否则为 `errno` 变量的值。这对支持如异步连接很有用。

  引发一个 审计事件 `socket.connect`，附带参数 `self`、`address`。

`socket.``detach`()

  将套接字对象置于关闭状态，而底层的文件描述符实际并不关闭。返回该文件描述符，使其可以重新用于其他目的。

  3.2 新版功能.

`socket.``dup`()

  创建套接字的副本。

  新创建的套接字是 不可继承的。

  在 3.4 版更改: 该套接字现在是不可继承的。

`socket.``fileno`()

  返回套接字的文件描述符（一个小整数），失败返回 -1。配合 `select.select()` 使用很有用。

  在 Windows 下，此方法返回的小整数在允许使用文件描述符的地方无法使用（如 `os.fdopen()` ）。Unix 无此限制。

`socket.``get_inheritable`()

  获取套接字文件描述符或套接字句柄的 可继承标志 ：如果子进程可以继承套接字则为 `True`，否则为 `False`。

  3.4 新版功能.

`socket.``getpeername`()

  返回套接字连接到的远程地址。举例而言，这可以用于查找远程 IPv4/v6 套接字的端口号。（返回的地址格式取决于地址簇 —— 参见上文。）部分系统不支持此函数。

`socket.``getsockname`()

  返回套接字本身的地址。举例而言，这可以用于查找 IPv4/v6 套接字的端口号。（返回的地址格式取决于地址簇 —— 参见上文。）

`socket.``getsockopt`(level, optname[, buflen])

  Return the value of the given socket option (see the Unix man page getsockopt(2)). The needed symbolic constants (`SO_*` etc.) are defined in this module. If buflen is absent, an integer option is assumed and its integer value is returned by the function. If buflen is present, it specifies the maximum length of the buffer used to receive the option in, and this buffer is returned as a bytes object. It is up to the caller to decode the contents of the buffer (see the optional built-in module `struct` for a way to decode C structures encoded as byte strings).

`socket.``getblocking`()

  Return `True` if socket is in blocking mode, `False` if in non-blocking.

  This is equivalent to checking `socket.gettimeout() == 0`.

  3.7 新版功能.

`socket.``gettimeout`()

  Return the timeout in seconds (float) associated with socket operations, or `None` if no timeout is set. This reflects the last call to `setblocking()` or `settimeout()`.

`socket.``ioctl`(control, option)
  Platform

    Windows

  The `ioctl()` method is a limited interface to the WSAIoctl system interface. Please refer to the Win32 documentation for more information.

  On other platforms, the generic `fcntl.fcntl()` and `fcntl.ioctl()` functions may be used; they accept a socket object as their first argument.

  Currently only the following control codes are supported: `SIO_RCVALL`, `SIO_KEEPALIVE_VALS`, and `SIO_LOOPBACK_FAST_PATH`.

  在 3.6 版更改: 添加了 `SIO_LOOPBACK_FAST_PATH`。

`socket.``listen`([backlog])

  Enable a server to accept connections. If backlog is specified, it must be at least 0 (if it is lower, it is set to 0); it specifies the number of unaccepted connections that the system will allow before refusing new connections. If not specified, a default reasonable value is chosen.

  在 3.5 版更改: The backlog parameter is now optional.

`socket.``makefile`(mode='r', buffering=None, *, encoding=None, errors=None, newline=None)

  Return a file object associated with the socket. The exact returned type depends on the arguments given to `makefile()`. These arguments are interpreted the same way as by the built-in `open()` function, except the only supported mode values are `'r'` (default), `'w'` and `'b'`.

  The socket must be in blocking mode; it can have a timeout, but the file object's internal buffer may end up in an inconsistent state if a timeout occurs.

  Closing the file object returned by `makefile()` won't close the original socket unless all other file objects have been closed and `socket.close()` has been called on the socket object.

  注解

  On Windows, the file-like object created by `makefile()` cannot be used where a file object with a file descriptor is expected, such as the stream arguments of `subprocess.Popen()`.

`socket.``recv`(bufsize[, flags])

  Receive data from the socket. The return value is a bytes object representing the data received. The maximum amount of data to be received at once is specified by bufsize. See the Unix manual page recv(2) for the meaning of the optional argument flags; it defaults to zero.

  注解

  For best match with hardware and network realities, the value of bufsize should be a relatively small power of 2, for example, 4096.

  在 3.5 版更改: 如果系统调用被中断，但信号处理程序没有触发异常，此方法现在会重试系统调用，而不是触发 `InterruptedError` 异常 (原因详见 PEP 475)。

`socket.``recvfrom`(bufsize[, flags])

  Receive data from the socket. The return value is a pair `(bytes, address)` where bytes is a bytes object representing the data received and address is the address of the socket sending the data. See the Unix manual page recv(2) for the meaning of the optional argument flags; it defaults to zero. (The format of address depends on the address family --- see above.)

  在 3.5 版更改: 如果系统调用被中断，但信号处理程序没有触发异常，此方法现在会重试系统调用，而不是触发 `InterruptedError` 异常 (原因详见 PEP 475)。

  在 3.7 版更改: For multicast IPv6 address, first item of address does not contain `%scope_id` part anymore. In order to get full IPv6 address use `getnameinfo()`.

`socket.``recvmsg`(bufsize[, ancbufsize[, flags]])

  Receive normal data (up to bufsize bytes) and ancillary data from the socket. The ancbufsize argument sets the size in bytes of the internal buffer used to receive the ancillary data; it defaults to 0, meaning that no ancillary data will be received. Appropriate buffer sizes for ancillary data can be calculated using `CMSG_SPACE()` or `CMSG_LEN()`, and items which do not fit into the buffer might be truncated or discarded. The flags argument defaults to 0 and has the same meaning as for `recv()`.

  The return value is a 4-tuple: `(data, ancdata, msg_flags, address)`. The data item is a `bytes` object holding the non-ancillary data received. The ancdata item is a list of zero or more tuples `(cmsg_level, cmsg_type, cmsg_data)` representing the ancillary data (control messages) received: cmsg_level and cmsg_type are integers specifying the protocol level and protocol-specific type respectively, and cmsg_data is a `bytes` object holding the associated data. The msg_flags item is the bitwise OR of various flags indicating conditions on the received message; see your system documentation for details. If the receiving socket is unconnected, address is the address of the sending socket, if available; otherwise, its value is unspecified.

  On some systems, `sendmsg()` and `recvmsg()` can be used to pass file descriptors between processes over an `AF_UNIX` socket. When this facility is used (it is often restricted to `SOCK_STREAM` sockets), `recvmsg()` will return, in its ancillary data, items of the form `(socket.SOL_SOCKET, socket.SCM_RIGHTS, fds)`, where fds is a `bytes` object representing the new file descriptors as a binary array of the native C `int` type. If `recvmsg()` raises an exception after the system call returns, it will first attempt to close any file descriptors received via this mechanism.

  Some systems do not indicate the truncated length of ancillary data items which have been only partially received. If an item appears to extend beyond the end of the buffer, `recvmsg()` will issue a `RuntimeWarning`, and will return the part of it which is inside the buffer provided it has not been truncated before the start of its associated data.

  On systems which support the `SCM_RIGHTS` mechanism, the following function will receive up to maxfds file descriptors, returning the message data and a list containing the descriptors (while ignoring unexpected conditions such as unrelated control messages being received). See also `sendmsg()`.

      import socket, array

      def recv_fds(sock, msglen, maxfds):
          fds = array.array("i")   # Array of ints
          msg, ancdata, flags, addr = sock.recvmsg(msglen, socket.CMSG_LEN(maxfds * fds.itemsize))
          for cmsg_level, cmsg_type, cmsg_data in ancdata:
              if cmsg_level == socket.SOL_SOCKET and cmsg_type == socket.SCM_RIGHTS:
                  # Append data, ignoring any truncated integers at the end.
                  fds.frombytes(cmsg_data[:len(cmsg_data) - (len(cmsg_data) % fds.itemsize)])
          return msg, list(fds)

  可用性： 大多数 Unix 平台，其他平台也可能可用。

  3.3 新版功能.

  在 3.5 版更改: 如果系统调用被中断，但信号处理程序没有触发异常，此方法现在会重试系统调用，而不是触发 `InterruptedError` 异常 (原因详见 PEP 475)。

`socket.``recvmsg_into`(buffers[, ancbufsize[, flags]])

  Receive normal data and ancillary data from the socket, behaving as `recvmsg()` would, but scatter the non-ancillary data into a series of buffers instead of returning a new bytes object. The buffers argument must be an iterable of objects that export writable buffers (e.g. `bytearray` objects); these will be filled with successive chunks of the non-ancillary data until it has all been written or there are no more buffers. The operating system may set a limit (`sysconf()` value `SC_IOV_MAX`) on the number of buffers that can be used. The ancbufsize and flags arguments have the same meaning as for `recvmsg()`.

  The return value is a 4-tuple: `(nbytes, ancdata, msg_flags, address)`, where nbytes is the total number of bytes of non-ancillary data written into the buffers, and ancdata, msg_flags and address are the same as for `recvmsg()`.

  示例:

      >>> import socket
      >>> s1, s2 = socket.socketpair()
      >>> b1 = bytearray(b'----')
      >>> b2 = bytearray(b'0123456789')
      >>> b3 = bytearray(b'--------------')
      >>> s1.send(b'Mary had a little lamb')
      22
      >>> s2.recvmsg_into([b1, memoryview(b2)[2:9], b3])
      (22, [], 0, None)
      >>> [b1, b2, b3]
      [bytearray(b'Mary'), bytearray(b'01 had a 9'), bytearray(b'little lamb---')]

  可用性： 大多数 Unix 平台，其他平台也可能可用。

  3.3 新版功能.

`socket.``recvfrom_into`(buffer[, nbytes[, flags]])

  Receive data from the socket, writing it into buffer instead of creating a new bytestring. The return value is a pair `(nbytes, address)` where nbytes is the number of bytes received and address is the address of the socket sending the data. See the Unix manual page recv(2) for the meaning of the optional argument flags; it defaults to zero. (The format of address depends on the address family --- see above.)

`socket.``recv_into`(buffer[, nbytes[, flags]])

  Receive up to nbytes bytes from the socket, storing the data into a buffer rather than creating a new bytestring. If nbytes is not specified (or 0), receive up to the size available in the given buffer. Returns the number of bytes received. See the Unix manual page recv(2) for the meaning of the optional argument flags; it defaults to zero.

`socket.``send`(bytes[, flags])

  Send data to the socket. The socket must be connected to a remote socket. The optional flags argument has the same meaning as for `recv()` above. Returns the number of bytes sent. Applications are responsible for checking that all data has been sent; if only some of the data was transmitted, the application needs to attempt delivery of the remaining data. For further information on this topic, consult the 套接字编程指南.

  在 3.5 版更改: 如果系统调用被中断，但信号处理程序没有触发异常，此方法现在会重试系统调用，而不是触发 `InterruptedError` 异常 (原因详见 PEP 475)。

`socket.``sendall`(bytes[, flags])

  Send data to the socket. The socket must be connected to a remote socket. The optional flags argument has the same meaning as for `recv()` above. Unlike `send()`, this method continues to send data from bytes until either all data has been sent or an error occurs. `None` is returned on success. On error, an exception is raised, and there is no way to determine how much data, if any, was successfully sent.

  在 3.5 版更改: The socket timeout is no more reset each time data is sent successfully. The socket timeout is now the maximum total duration to send all data.

  在 3.5 版更改: 如果系统调用被中断，但信号处理程序没有触发异常，此方法现在会重试系统调用，而不是触发 `InterruptedError` 异常 (原因详见 PEP 475)。

`socket.``sendto`(bytes, address)
`socket.``sendto`(bytes, flags, address)

  Send data to the socket. The socket should not be connected to a remote socket, since the destination socket is specified by address. The optional flags argument has the same meaning as for `recv()` above. Return the number of bytes sent. (The format of address depends on the address family --- see above.)

  引发一个 审计事件 `socket.sendto`，附带参数 `self`、`address`。

  在 3.5 版更改: 如果系统调用被中断，但信号处理程序没有触发异常，此方法现在会重试系统调用，而不是触发 `InterruptedError` 异常 (原因详见 PEP 475)。

`socket.``sendmsg`(buffers[, ancdata[, flags[, address]]])

  Send normal and ancillary data to the socket, gathering the non-ancillary data from a series of buffers and concatenating it into a single message. The buffers argument specifies the non-ancillary data as an iterable of bytes-like objects (e.g. `bytes` objects); the operating system may set a limit (`sysconf()` value `SC_IOV_MAX`) on the number of buffers that can be used. The ancdata argument specifies the ancillary data (control messages) as an iterable of zero or more tuples `(cmsg_level, cmsg_type, cmsg_data)`, where cmsg_level and cmsg_type are integers specifying the protocol level and protocol-specific type respectively, and cmsg_data is a bytes-like object holding the associated data. Note that some systems (in particular, systems without `CMSG_SPACE()`) might support sending only one control message per call. The flags argument defaults to 0 and has the same meaning as for `send()`. If address is supplied and not `None`, it sets a destination address for the message. The return value is the number of bytes of non-ancillary data sent.

  The following function sends the list of file descriptors fds over an `AF_UNIX` socket, on systems which support the `SCM_RIGHTS` mechanism. See also `recvmsg()`.

      import socket, array

      def send_fds(sock, msg, fds):
          return sock.sendmsg([msg], [(socket.SOL_SOCKET, socket.SCM_RIGHTS, array.array("i", fds))])

  可用性： 大多数 Unix 平台，其他平台也可能可用。

  引发一个 审计事件 `socket.sendmsg`，附带参数 `self`、`address`。

  3.3 新版功能.

  在 3.5 版更改: 如果系统调用被中断，但信号处理程序没有触发异常，此方法现在会重试系统调用，而不是触发 `InterruptedError` 异常 (原因详见 PEP 475)。

`socket.``sendmsg_afalg`([msg, ]*, op[, iv[, assoclen[, flags]]])

  Specialized version of `sendmsg()` for `AF_ALG` socket. Set mode, IV, AEAD associated data length and flags for `AF_ALG` socket.

  可用性： Linux >= 2.6.38。

  3.6 新版功能.

`socket.``send_fds`(sock, buffers, fds[, flags[, address]])

  Send the list of file descriptors fds over an `AF_UNIX` socket. The fds parameter is a sequence of file descriptors. Consult `sendmsg()` for the documentation of these parameters.

  Availability: Unix supporting `sendmsg()` and `SCM_RIGHTS` mechanism.

  3.9 新版功能.

`socket.``recv_fds`(sock, bufsize, maxfds[, flags])

  Receive up to maxfds file descriptors. Return `(msg, list(fds), flags, addr)`. Consult `recvmsg()` for the documentation of these parameters.

  Availability: Unix supporting `recvmsg()` and `SCM_RIGHTS` mechanism.

  3.9 新版功能.

  注解

  Any truncated integers at the end of the list of file descriptors.

`socket.``sendfile`(file, offset=0, count=None)

  Send a file until EOF is reached by using high-performance `os.sendfile` and return the total number of bytes which were sent. file must be a regular file object opened in binary mode. If `os.sendfile` is not available (e.g. Windows) or file is not a regular file `send()` will be used instead. offset tells from where to start reading the file. If specified, count is the total number of bytes to transmit as opposed to sending the file until EOF is reached. File position is updated on return or also in case of error in which case `file.tell()` can be used to figure out the number of bytes which were sent. The socket must be of `SOCK_STREAM` type. Non-blocking sockets are not supported.

  3.5 新版功能.

`socket.``set_inheritable`(inheritable)

  Set the inheritable flag of the socket's file descriptor or socket's handle.

  3.4 新版功能.

`socket.``setblocking`(flag)

  Set blocking or non-blocking mode of the socket: if flag is false, the socket is set to non-blocking, else to blocking mode.

  This method is a shorthand for certain `settimeout()` calls:

  - `sock.setblocking(True)` is equivalent to `sock.settimeout(None)`

  - `sock.setblocking(False)` is equivalent to `sock.settimeout(0.0)`

  在 3.7 版更改: The method no longer applies `SOCK_NONBLOCK` flag on `socket.type`.

`socket.``settimeout`(value)

  Set a timeout on blocking socket operations. The value argument can be a nonnegative floating point number expressing seconds, or `None`. If a non-zero value is given, subsequent socket operations will raise a `timeout` exception if the timeout period value has elapsed before the operation has completed. If zero is given, the socket is put in non-blocking mode. If `None` is given, the socket is put in blocking mode.

  For further information, please consult the notes on socket timeouts.

  在 3.7 版更改: The method no longer toggles `SOCK_NONBLOCK` flag on `socket.type`.

`socket.``setsockopt`(level, optname, value: int)

`socket.``setsockopt`(level, optname, value: buffer)

`socket.``setsockopt`(level, optname, None, optlen: int)

  Set the value of the given socket option (see the Unix manual page setsockopt(2)). The needed symbolic constants are defined in the `socket` module (`SO_*` etc.). The value can be an integer, `None` or a bytes-like object representing a buffer. In the later case it is up to the caller to ensure that the bytestring contains the proper bits (see the optional built-in module `struct` for a way to encode C structures as bytestrings). When value is set to `None`, optlen argument is required. It's equivalent to call `setsockopt()` C function with `optval=NULL` and `optlen=optlen`.

  在 3.5 版更改: 现在支持可写的 字节类对象。

  在 3.6 版更改: setsockopt(level, optname, None, optlen: int) form added.

`socket.``shutdown`(how)

  Shut down one or both halves of the connection. If how is `SHUT_RD`, further receives are disallowed. If how is `SHUT_WR`, further sends are disallowed. If how is `SHUT_RDWR`, further sends and receives are disallowed.

`socket.``share`(process_id)

  Duplicate a socket and prepare it for sharing with a target process. The target process must be provided with process_id. The resulting bytes object can then be passed to the target process using some form of interprocess communication and the socket can be recreated there using `fromshare()`. Once this method has been called, it is safe to close the socket since the operating system has already duplicated it for the target process.

  可用性: Windows。

  3.3 新版功能.

Note that there are no methods `read()` or `write()`; use `recv()` and `send()` without flags argument instead.

Socket objects also have these (read-only) attributes that correspond to the values given to the `socket` constructor.

`socket.``family`

  The socket family.

`socket.``type`

  The socket type.

`socket.``proto`

  The socket protocol.

## Notes on socket timeouts

A socket object can be in one of three modes: blocking, non-blocking, or timeout. Sockets are by default always created in blocking mode, but this can be changed by calling `setdefaulttimeout()`.

- In blocking mode, operations block until complete or the system returns an error (such as connection timed out).

- In non-blocking mode, operations fail (with an error that is unfortunately system-dependent) if they cannot be completed immediately: functions from the `select` can be used to know when and whether a socket is available for reading or writing.

- In timeout mode, operations fail if they cannot be completed within the timeout specified for the socket (they raise a `timeout` exception) or if the system returns an error.

注解

At the operating system level, sockets in timeout mode are internally set in non-blocking mode. Also, the blocking and timeout modes are shared between file descriptors and socket objects that refer to the same network endpoint. This implementation detail can have visible consequences if e.g. you decide to use the `fileno()` of a socket.

### Timeouts and the `connect` method

The `connect()` operation is also subject to the timeout setting, and in general it is recommended to call `settimeout()` before calling `connect()` or pass a timeout parameter to `create_connection()`. However, the system network stack may also return a connection timeout error of its own regardless of any Python socket timeout setting.

### Timeouts and the `accept` method

If `getdefaulttimeout()` is not `None`, sockets returned by the `accept()` method inherit that timeout. Otherwise, the behaviour depends on settings of the listening socket:

- if the listening socket is in blocking mode or in timeout mode, the socket returned by `accept()` is in blocking mode;

- if the listening socket is in non-blocking mode, whether the socket returned by `accept()` is in blocking or non-blocking mode is operating system-dependent. If you want to ensure cross-platform behaviour, it is recommended you manually override this setting.

## 示例

Here are four minimal example programs using the TCP/IP protocol: a server that echoes all data that it receives back (servicing only one client), and a client using it. Note that a server must perform the sequence `socket()`, `bind()`, `listen()`, `accept()` (possibly repeating the `accept()` to service more than one client), while a client only needs the sequence `socket()`, `connect()`. Also note that the server does not `sendall()`/`recv()` on the socket it is listening on but on the new socket returned by `accept()`.

The first two examples support IPv4 only.

    # Echo server program
    import socket

    HOST = ''                 # Symbolic name meaning all available interfaces
    PORT = 50007              # Arbitrary non-privileged port
    with socket.socket(socket.AF_INET, socket.SOCK_STREAM) as s:
        s.bind((HOST, PORT))
        s.listen(1)
        conn, addr = s.accept()
        with conn:
            print('Connected by', addr)
            while True:
                data = conn.recv(1024)
                if not data: break
                conn.sendall(data)

    # Echo client program
    import socket

    HOST = 'daring.cwi.nl'    # The remote host
    PORT = 50007              # The same port as used by the server
    with socket.socket(socket.AF_INET, socket.SOCK_STREAM) as s:
        s.connect((HOST, PORT))
        s.sendall(b'Hello, world')
        data = s.recv(1024)
    print('Received', repr(data))

The next two examples are identical to the above two, but support both IPv4 and IPv6. The server side will listen to the first address family available (it should listen to both instead). On most of IPv6-ready systems, IPv6 will take precedence and the server may not accept IPv4 traffic. The client side will try to connect to the all addresses returned as a result of the name resolution, and sends traffic to the first one connected successfully.

    # Echo server program
    import socket
    import sys

    HOST = None               # Symbolic name meaning all available interfaces
    PORT = 50007              # Arbitrary non-privileged port
    s = None
    for res in socket.getaddrinfo(HOST, PORT, socket.AF_UNSPEC,
                                  socket.SOCK_STREAM, 0, socket.AI_PASSIVE):
        af, socktype, proto, canonname, sa = res
        try:
            s = socket.socket(af, socktype, proto)
        except OSError as msg:
            s = None
            continue
        try:
            s.bind(sa)
            s.listen(1)
        except OSError as msg:
            s.close()
            s = None
            continue
        break
    if s is None:
        print('could not open socket')
        sys.exit(1)
    conn, addr = s.accept()
    with conn:
        print('Connected by', addr)
        while True:
            data = conn.recv(1024)
            if not data: break
            conn.send(data)

    # Echo client program
    import socket
    import sys

    HOST = 'daring.cwi.nl'    # The remote host
    PORT = 50007              # The same port as used by the server
    s = None
    for res in socket.getaddrinfo(HOST, PORT, socket.AF_UNSPEC, socket.SOCK_STREAM):
        af, socktype, proto, canonname, sa = res
        try:
            s = socket.socket(af, socktype, proto)
        except OSError as msg:
            s = None
            continue
        try:
            s.connect(sa)
        except OSError as msg:
            s.close()
            s = None
            continue
        break
    if s is None:
        print('could not open socket')
        sys.exit(1)
    with s:
        s.sendall(b'Hello, world')
        data = s.recv(1024)
    print('Received', repr(data))

The next example shows how to write a very simple network sniffer with raw sockets on Windows. The example requires administrator privileges to modify the interface:

    import socket

    # the public network interface
    HOST = socket.gethostbyname(socket.gethostname())

    # create a raw socket and bind it to the public interface
    s = socket.socket(socket.AF_INET, socket.SOCK_RAW, socket.IPPROTO_IP)
    s.bind((HOST, 0))

    # Include IP headers
    s.setsockopt(socket.IPPROTO_IP, socket.IP_HDRINCL, 1)

    # receive all packages
    s.ioctl(socket.SIO_RCVALL, socket.RCVALL_ON)

    # receive a package
    print(s.recvfrom(65565))

    # disabled promiscuous mode
    s.ioctl(socket.SIO_RCVALL, socket.RCVALL_OFF)

The next example shows how to use the socket interface to communicate to a CAN network using the raw socket protocol. To use CAN with the broadcast manager protocol instead, open a socket with:

    socket.socket(socket.AF_CAN, socket.SOCK_DGRAM, socket.CAN_BCM)

After binding (`CAN_RAW`) or connecting (`CAN_BCM`) the socket, you can use the `socket.send()`, and the `socket.recv()` operations (and their counterparts) on the socket object as usual.

This last example might require special privileges:

    import socket
    import struct

    # CAN frame packing/unpacking (see 'struct can_frame' in <linux/can.h>)

    can_frame_fmt = "=IB3x8s"
    can_frame_size = struct.calcsize(can_frame_fmt)

    def build_can_frame(can_id, data):
        can_dlc = len(data)
        data = data.ljust(8, b'\x00')
        return struct.pack(can_frame_fmt, can_id, can_dlc, data)

    def dissect_can_frame(frame):
        can_id, can_dlc, data = struct.unpack(can_frame_fmt, frame)
        return (can_id, can_dlc, data[:can_dlc])

    # create a raw socket and bind it to the 'vcan0' interface
    s = socket.socket(socket.AF_CAN, socket.SOCK_RAW, socket.CAN_RAW)
    s.bind(('vcan0',))

    while True:
        cf, addr = s.recvfrom(can_frame_size)

        print('Received: can_id=%x, can_dlc=%x, data=%s' % dissect_can_frame(cf))

        try:
            s.send(cf)
        except OSError:
            print('Error sending CAN frame')

        try:
            s.send(build_can_frame(0x01, b'\x01\x02\x03'))
        except OSError:
            print('Error sending CAN frame')

Running an example several times with too small delay between executions, could lead to this error:

    OSError: [Errno 98] Address already in use

This is because the previous execution has left the socket in a `TIME_WAIT` state, and can't be immediately reused.

There is a `socket` flag to set, in order to prevent this, `socket.SO_REUSEADDR`:

    s = socket.socket(socket.AF_INET, socket.SOCK_STREAM)
    s.setsockopt(socket.SOL_SOCKET, socket.SO_REUSEADDR, 1)
    s.bind((HOST, PORT))

the `SO_REUSEADDR` flag tells the kernel to reuse a local socket in `TIME_WAIT` state, without waiting for its natural timeout to expire.

参见

For an introduction to socket programming (in C), see the following papers:

- An Introductory 4.3BSD Interprocess Communication Tutorial, by Stuart Sechrest

- An Advanced 4.3BSD Interprocess Communication Tutorial, by Samuel J. Leffler et al,

both in the UNIX Programmer's Manual, Supplementary Documents 1 (sections PS1:7 and PS1:8). The platform-specific reference material for the various socket-related system calls are also a valuable source of information on the details of socket semantics. For Unix, refer to the manual pages; for Windows, see the WinSock (or Winsock 2) specification. For IPv6-ready APIs, readers may want to refer to RFC 3493 titled Basic Socket Interface Extensions for IPv6.