28.16. "fpectl" — Floating point exception control
**************************************************

備註: The "fpectl" module is not built by default, and its usage is
  discouraged and may be dangerous except in the hands of experts. See
  also the section Limitations and other considerations on limitations
  for more details.

Most computers carry out floating point operations in conformance with
the so-called IEEE-754 standard. On any real computer, some floating
point operations produce results that cannot be expressed as a normal
floating point value. For example, try

   >>> import math
   >>> math.exp(1000)
   inf
   >>> math.exp(1000) / math.exp(1000)
   nan

(The example above will work on many platforms. DEC Alpha may be one
exception.) 「Inf」 is a special, non-numeric value in IEEE-754 that
stands for 「infinity」, and 「nan」 means 「not a number.」 Note
that, other than the non-numeric results, nothing special happened
when you asked Python to carry out those calculations. That is in fact
the default behaviour prescribed in the IEEE-754 standard, and if it
works for you, stop reading now.

In some circumstances, it would be better to raise an exception and
stop processing at the point where the faulty operation was attempted.
The "fpectl" module is for use in that situation. It provides control
over floating point units from several hardware manufacturers,
allowing the user to turn on the generation of "SIGFPE" whenever any
of the IEEE-754 exceptions Division by Zero, Overflow, or Invalid
Operation occurs. In tandem with a pair of wrapper macros that are
inserted into the C code comprising your python system, "SIGFPE" is
trapped and converted into the Python "FloatingPointError" exception.

The "fpectl" module defines the following functions and may raise the
given exception:

fpectl.turnon_sigfpe()

   Turn on the generation of "SIGFPE", and set up an appropriate
   signal handler.

fpectl.turnoff_sigfpe()

   Reset default handling of floating point exceptions.

exception fpectl.FloatingPointError

   After "turnon_sigfpe()" has been executed, a floating point
   operation that raises one of the IEEE-754 exceptions Division by
   Zero, Overflow, or Invalid operation will in turn raise this
   standard Python exception.


28.16.1. Example
================

The following example demonstrates how to start up and test operation
of the "fpectl" module.

   >>> import fpectl
   >>> import fpetest
   >>> fpectl.turnon_sigfpe()
   >>> fpetest.test()
   overflow        PASS
   FloatingPointError: Overflow

   div by 0        PASS
   FloatingPointError: Division by zero
     [ more output from test elided ]
   >>> import math
   >>> math.exp(1000)
   Traceback (most recent call last):
     File "<stdin>", line 1, in <module>
   FloatingPointError: in math_1


28.16.2. Limitations and other considerations
=============================================

Setting up a given processor to trap IEEE-754 floating point errors
currently requires custom code on a per-architecture basis. You may
have to modify "fpectl" to control your particular hardware.

Conversion of an IEEE-754 exception to a Python exception requires
that the wrapper macros "PyFPE_START_PROTECT" and "PyFPE_END_PROTECT"
be inserted into your code in an appropriate fashion.  Python itself
has been modified to support the "fpectl" module, but many other codes
of interest to numerical analysts have not.

The "fpectl" module is not thread-safe.

也參考: Some files in the source distribution may be interesting in
  learning more about how this module operates. The include file
  Include/pyfpe.h discusses the implementation of this module at some
  length. Modules/fpetestmodule.c gives several examples of use. Many
  additional examples can be found in Objects/floatobject.c.
